ID      |Generation Time     |Severity    |Event Code  |Status      |Event Description
100     |2026-04-01 10:42:24 |Normal      |0x1A00006F  |Asserted    |The openUBMC is reset, with the cause code of 0x2.
99      |2026-04-01 10:42:19 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
98      |2026-04-01 10:21:05 |Normal      |0x1A00006F  |Asserted    |The openUBMC is reset, with the cause code of 0x2.
97      |2026-04-01 10:21:03 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
96      |2026-04-01 10:07:10 |Normal      |0x1A00006F  |Asserted    |The openUBMC is reset, with the cause code of 0x2.
95      |2026-04-01 10:07:09 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
94      |2026-04-01 09:50:28 |Normal      |0x1A00006F  |Asserted    |The openUBMC is reset, with the cause code of 0x2.
93      |2026-04-01 09:50:26 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
92      |2026-04-01 09:19:22 |Normal      |0x1A00002C  |Deasserted  |openUBMC failed to synchronize time with the NTP server.
91      |2026-04-01 09:17:19 |Normal      |0x1A00002B  |Asserted    |openUBMC failed to synchronize time with the NTP server.
90      |2026-04-01 08:53:57 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
89      |2026-04-01 08:53:56 |Normal      |0x1A00006F  |Asserted    |The openUBMC is reset, with the cause code of 0x2.
88      |2026-04-01 08:38:58 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
87      |2026-04-01 08:34:30 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
86      |2026-04-01 08:30:02 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
85      |2026-04-01 08:25:48 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
84      |2026-04-01 08:21:52 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
83      |2026-04-01 08:18:36 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
82      |2026-04-01 08:18:31 |Normal      |0x04000003  |Asserted    |Fan 5 removed.
81      |2026-04-01 08:18:30 |Major       |0x2400000D  |Asserted    |CPU board voltage ( V) at 3.3V detection point BCU_V_VCC_3V3 is lower than the undervoltage threshold (3.0 V) (SN:1025B6860740).
80      |2026-04-01 08:18:29 |Major       |0x2400000D  |Asserted    |CPU board voltage (0.680 V) at 0.9V detection point BCU_V_VCC_0V9 is lower than the undervoltage threshold (0.8 V) (SN:1025B6860740).
79      |2026-04-01 08:18:28 |Normal      |0x04000001  |Asserted    |Fan 5 installed.
78      |2026-04-01 08:18:15 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
77      |2026-04-01 08:18:12 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
76      |2026-04-01 08:08:50 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
75      |2026-04-01 08:04:28 |Normal      |0x1A00006F  |Asserted    |The openUBMC is reset, with the cause code of 0x2.
74      |2026-04-01 08:04:27 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
73      |2026-04-01 07:32:38 |Major       |0x24000010  |Deasserted  |CPU board voltage (15.000 V) at 12V detection point BCU_V_12V0_IN_COPPER exceeds the overvoltage threshold (13.2 V) (SN:1025B6860762).
72      |2026-04-01 07:32:37 |Major       |0x2400000E  |Deasserted  |CPU board voltage ( V) at 3.3V detection point BCU_V_VCC_3V3 is lower than the undervoltage threshold (3.0 V) (SN:1025B6860762).
71      |2026-04-01 07:32:37 |Major       |0x2400000E  |Deasserted  |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER is lower than the undervoltage threshold (3.0 V) (SN:1025B6860762).
70      |2026-04-01 07:32:37 |Major       |0x24000010  |Deasserted  |CPU board voltage ( V) at 0.9V detection point BCU_V_VCC_0V9 exceeds the overvoltage threshold (1.0 V) (SN:1025B6860762).
69      |2026-04-01 07:32:26 |Major       |0x2400000D  |Asserted    |CPU board voltage ( V) at 3.3V detection point BCU_V_VCC_3V3 is lower than the undervoltage threshold (3.0 V) (SN:1025B6860762).
68      |2026-04-01 07:32:26 |Major       |0x24000010  |Deasserted  |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
67      |2026-04-01 07:32:25 |Major       |0x24000010  |Deasserted  |CPU board voltage (2.500 V) at 1.8V detection point BCU_V_VCC_1V8 exceeds the overvoltage threshold (2.0 V) (SN:1025B6860740).
66      |2026-04-01 07:32:25 |Major       |0x24000010  |Deasserted  |CPU board voltage (2.500 V) at 1.8V detection point BCU_V_VCC_1V8 exceeds the overvoltage threshold (2.0 V) (SN:1025B6860762).
65      |2026-04-01 07:32:25 |Major       |0x24000010  |Deasserted  |CPU board voltage (5.000 V) at 3.3V detection point BCU_V_VCC_3V3 exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
64      |2026-04-01 07:32:25 |Major       |0x2400000D  |Asserted    |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER is lower than the undervoltage threshold (3.0 V) (SN:1025B6860762).
63      |2026-04-01 07:32:22 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
62      |2026-04-01 07:32:21 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
61      |2026-04-01 07:32:18 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
60      |2026-04-01 07:27:58 |Major       |0x2400000F  |Asserted    |CPU board voltage (2.500 V) at 1.8V detection point BCU_V_VCC_1V8 exceeds the overvoltage threshold (2.0 V) (SN:1025B6860740).
59      |2026-04-01 07:26:58 |Major       |0x2400000F  |Asserted    |CPU board voltage ( V) at 0.9V detection point BCU_V_VCC_0V9 exceeds the overvoltage threshold (1.0 V) (SN:1025B6860762).
58      |2026-04-01 07:26:58 |Major       |0x2400000F  |Asserted    |CPU board voltage (15.000 V) at 12V detection point BCU_V_12V0_IN_COPPER exceeds the overvoltage threshold (13.2 V) (SN:1025B6860762).
57      |2026-04-01 07:25:57 |Major       |0x2400000F  |Asserted    |CPU board voltage (5.000 V) at 3.3V detection point BCU_V_VCC_3V3 exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
56      |2026-04-01 07:25:57 |Major       |0x2400000F  |Asserted    |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
55      |2026-04-01 07:22:57 |Major       |0x2400000F  |Asserted    |CPU board voltage (2.500 V) at 1.8V detection point BCU_V_VCC_1V8 exceeds the overvoltage threshold (2.0 V) (SN:1025B6860762).
54      |2026-04-01 07:16:56 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
53      |2026-04-01 06:52:35 |Major       |0x2400000F  |Asserted    |CPU board voltage (15.000 V) at 12V detection point BCU_V_12V0_IN_COPPER exceeds the overvoltage threshold (13.2 V) (SN:1025B6860762).
52      |2026-04-01 06:52:31 |Major       |0x24000010  |Deasserted  |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
51      |2026-04-01 06:52:31 |Major       |0x24000010  |Deasserted  |CPU board voltage (2.500 V) at 1.8V detection point BCU_V_VCC_1V8 exceeds the overvoltage threshold (2.0 V) (SN:1025B6860762).
50      |2026-04-01 06:52:31 |Major       |0x24000010  |Deasserted  |CPU board voltage ( V) at 0.9V detection point BCU_V_VCC_0V9 exceeds the overvoltage threshold (1.0 V) (SN:1025B6860762).
49      |2026-04-01 06:52:30 |Major       |0x2400000E  |Deasserted  |CPU board voltage (0.037 V) at 1.8V detection point BCU_V_VCC_1V8 is lower than the undervoltage threshold (1.6 V) (SN:1025B6860762).
48      |2026-04-01 06:52:30 |Major       |0x2400000F  |Asserted    |CPU board voltage ( V) at 0.9V detection point BCU_V_VCC_0V9 exceeds the overvoltage threshold (1.0 V) (SN:1025B6860762).
47      |2026-04-01 06:52:30 |Major       |0x2400000F  |Asserted    |CPU board voltage (2.500 V) at 1.8V detection point BCU_V_VCC_1V8 exceeds the overvoltage threshold (2.0 V) (SN:1025B6860762).
46      |2026-04-01 06:52:30 |Major       |0x2400000F  |Asserted    |CPU board voltage (5.000 V) at 3.3V detection point BCU_V_VCC_3V3 exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
45      |2026-04-01 06:52:30 |Major       |0x2400000F  |Asserted    |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
44      |2026-04-01 06:52:29 |Major       |0x2400000E  |Deasserted  |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER is lower than the undervoltage threshold (3.0 V) (SN:1025B6860762).
43      |2026-04-01 06:52:29 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
42      |2026-04-01 06:52:28 |Major       |0x2400000D  |Asserted    |CPU board voltage (0.037 V) at 1.8V detection point BCU_V_VCC_1V8 is lower than the undervoltage threshold (1.6 V) (SN:1025B6860762).
41      |2026-04-01 06:52:27 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
40      |2026-04-01 06:52:25 |Major       |0x2400000D  |Asserted    |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER is lower than the undervoltage threshold (3.0 V) (SN:1025B6860762).
39      |2026-04-01 06:52:25 |Major       |0x24000010  |Deasserted  |CPU board voltage (2.500 V) at 1.8V detection point BCU_V_VCC_1V8 exceeds the overvoltage threshold (2.0 V) (SN:1025B6860762).
38      |2026-04-01 06:52:25 |Major       |0x24000010  |Deasserted  |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
37      |2026-04-01 06:52:24 |Major       |0x24000010  |Deasserted  |CPU board voltage (5.000 V) at 3.3V detection point BCU_V_VCC_3V3 exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
36      |2026-04-01 06:52:22 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
35      |2026-04-01 06:52:22 |Major       |0x24000010  |Deasserted  |CPU board voltage ( V) at 0.9V detection point BCU_V_VCC_0V9 exceeds the overvoltage threshold (1.0 V) (SN:1025B6860762).
34      |2026-04-01 06:52:21 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
33      |2026-04-01 06:52:17 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
32      |2026-04-01 06:48:32 |Major       |0x2400000F  |Asserted    |CPU board voltage (5.000 V) at 3.3V detection point BCU_V_VCC_3V3 exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
31      |2026-04-01 06:47:32 |Major       |0x2400000F  |Asserted    |CPU board voltage ( V) at 0.9V detection point BCU_V_VCC_0V9 exceeds the overvoltage threshold (1.0 V) (SN:1025B6860762).
30      |2026-04-01 06:47:32 |Major       |0x2400000F  |Asserted    |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
29      |2026-04-01 06:47:32 |Major       |0x2400000F  |Asserted    |CPU board voltage (2.500 V) at 1.8V detection point BCU_V_VCC_1V8 exceeds the overvoltage threshold (2.0 V) (SN:1025B6860762).
28      |2026-04-01 06:46:56 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
27      |2026-04-01 06:45:52 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
26      |2026-04-01 06:45:51 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
25      |2026-04-01 06:45:48 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
24      |2026-04-01 06:42:31 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
23      |2026-04-01 03:24:00 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
22      |2026-04-01 03:14:13 |Major       |0x2400000F  |Asserted    |CPU board voltage (5.000 V) at 3.3V detection point BCU_V_VCC_3V3 exceeds the overvoltage threshold (3.6 V) (SN:1025B6860740).
21      |2026-04-01 03:14:13 |Major       |0x2400000F  |Asserted    |CPU board voltage (2.500 V) at 1.8V detection point BCU_V_VCC_1V8 exceeds the overvoltage threshold (2.0 V) (SN:1025B6860740).
20      |2026-04-01 03:14:12 |Major       |0x2400000F  |Asserted    |CPU board voltage ( V) at 3.3V detection point BCU_V_STBY_3V3_RISER exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
19      |2026-04-01 03:14:12 |Major       |0x2400000F  |Asserted    |CPU board voltage (15.000 V) at 12V detection point BCU_V_12V0_IN_COPPER exceeds the overvoltage threshold (13.2 V) (SN:1025B6860762).
18      |2026-04-01 03:14:12 |Major       |0x2400000F  |Asserted    |CPU board voltage (2.500 V) at 1.8V detection point BCU_V_VCC_1V8 exceeds the overvoltage threshold (2.0 V) (SN:1025B6860762).
17      |2026-04-01 03:14:12 |Major       |0x2400000F  |Asserted    |CPU board voltage (5.000 V) at 3.3V detection point BCU_V_VCC_3V3 exceeds the overvoltage threshold (3.6 V) (SN:1025B6860762).
16      |2026-04-01 03:14:11 |Major       |0x2400000F  |Asserted    |CPU board voltage ( V) at 0.9V detection point BCU_V_VCC_0V9 exceeds the overvoltage threshold (1.0 V) (SN:1025B6860762).
15      |2026-04-01 03:05:41 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
14      |2026-04-01 03:05:38 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
13      |2026-04-01 03:05:38 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
12      |2026-04-01 03:05:37 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
11      |2026-04-01 03:04:21 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
10      |2026-04-01 03:04:10 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
9       |2026-04-01 03:04:08 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
8       |2026-04-01 02:14:42 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
7       |2026-04-01 02:11:17 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
6       |2026-04-01 02:08:06 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
5       |2026-03-31 19:54:37 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
4       |2026-03-31 19:52:17 |Normal      |0x1A00002C  |Deasserted  |openUBMC failed to synchronize time with the NTP server.
3       |2026-03-31 19:50:50 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
2       |2026-03-31 19:09:11 |Normal      |0x1A00002B  |Asserted    |openUBMC failed to synchronize time with the NTP server.
1       |2026-03-31 18:26:59 |Normal      |0x1A00000F  |Asserted    |openUBMC event records are cleared.
