ID      |Generation Time     |Severity    |Event Code  |Status      |Event Description
23      |2026-07-14 14:52:43 |Normal      |0x1A00006F  |Asserted    |The iBMC is reset, with the cause code of 0x2.
22      |2026-07-14 13:50:42 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
21      |2026-07-14 13:49:40 |Normal      |0x1A00006F  |Asserted    |The iBMC is reset, with the cause code of 0x2.
20      |2026-07-14 12:08:54 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
19      |2026-07-14 12:07:54 |Normal      |0x1A00006F  |Asserted    |The iBMC is reset, with the cause code of 0x2.
18      |2026-07-14 11:58:10 |Critical    |0x08000002  |Deasserted  |The PCIe Card 2 (LPe32002-AP) triggered an uncorrectable error. Error code: NA (SN:FP20114429, BN:LPe32002-M2-AP).
17      |2026-07-14 11:57:41 |Critical    |0x08000001  |Asserted    |The PCIe Card 2 (LPe32002-AP) triggered an uncorrectable error. Error code: NA (SN:FP20114429, BN:LPe32002-M2-AP).
16      |2026-07-14 11:55:26 |Normal      |0x08000066  |Deasserted  |PCIe Card 2 (LPe32002-AP) health status degradation detected by PFAE (SN:FP20114429, BN:LPe32002-M2-AP).
15      |2026-07-14 11:54:55 |Normal      |0x08000065  |Asserted    |PCIe Card 2 (LPe32002-AP) health status degradation detected by PFAE (SN:FP20114429, BN:LPe32002-M2-AP).
14      |2026-07-14 11:51:21 |Minor       |0x08000070  |Deasserted  |The PCIe card 2 (LPe32002-AP) bandwidth decreased (SN:FP20114429, BN:LPe32002-M2-AP).
13      |2026-07-14 11:50:23 |Minor       |0x0800006F  |Asserted    |The PCIe card 2 (LPe32002-AP) bandwidth decreased (SN:FP20114429, BN:LPe32002-M2-AP).
12      |2026-07-14 11:06:38 |Normal      |0x29000002  |Deasserted  |PCIe Card 2 (LPe32002-AP) Port 2 disconnected.
11      |2026-07-14 11:06:33 |Normal      |0x29000002  |Deasserted  |PCIe Card 2 (LPe32002-AP) Port 1 disconnected.
10      |2026-07-14 11:03:12 |Normal      |0x29000001  |Asserted    |PCIe Card 2 (LPe32002-AP) Port 2 disconnected.
9       |2026-07-14 11:00:40 |Normal      |0x29000001  |Asserted    |PCIe Card 2 (LPe32002-AP) Port 1 disconnected.
8       |2026-07-14 00:51:22 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF221Q) Port 1 disconnected.
7       |2026-07-14 00:50:58 |Normal      |0x29000002  |Deasserted  |PCIe Card 2 (LPe32002-AP) Port 1 disconnected.
6       |2026-07-14 00:50:58 |Normal      |0x29000002  |Deasserted  |PCIe Card 2 (LPe32002-AP) Port 2 disconnected.
5       |2026-07-14 00:48:27 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 1 disconnected.
4       |2026-07-14 00:48:17 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
3       |2026-07-14 00:48:13 |Normal      |0x29000001  |Asserted    |PCIe Card 2 (LPe32002-AP) Port 2 disconnected.
2       |2026-07-14 00:48:13 |Normal      |0x29000001  |Asserted    |PCIe Card 2 (LPe32002-AP) Port 1 disconnected.
1       |2026-07-14 00:47:54 |Normal      |0x1A00000F  |Asserted    |iBMC event records are cleared.
