ID      |Generation Time     |Severity    |Event Code  |Status      |Event Description
501     |2026-04-21 05:44:40 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
500     |2026-04-21 04:47:47 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
499     |2026-04-21 04:17:42 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
498     |2026-04-21 04:17:21 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
497     |2026-04-21 04:04:15 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
496     |2026-04-21 04:03:09 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
495     |2026-04-21 03:53:05 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
494     |2026-04-21 03:35:31 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
493     |2026-04-21 03:23:05 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
492     |2026-04-21 03:22:43 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
491     |2026-04-20 07:11:59 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
490     |2026-04-20 07:11:59 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
489     |2026-04-20 07:11:45 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
488     |2026-04-20 06:59:35 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
487     |2026-04-20 03:47:12 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
486     |2026-04-20 03:45:34 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
485     |2026-04-20 03:30:06 |Minor       |0x08000004  |Deasserted  |The PCIe Card 6 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001030).
484     |2026-04-20 03:27:15 |Minor       |0x08000003  |Asserted    |The PCIe Card 6 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001030).
483     |2026-04-20 03:22:06 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
482     |2026-04-20 03:18:57 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
481     |2026-04-20 03:16:12 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
480     |2026-04-20 03:08:38 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
479     |2026-04-20 03:07:42 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
478     |2026-04-20 02:58:25 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
477     |2026-04-20 02:58:03 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
476     |2026-04-20 02:43:53 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
475     |2026-04-20 02:41:58 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
474     |2026-04-20 02:32:29 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
473     |2026-04-20 02:31:32 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
472     |2026-04-16 17:53:42 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
471     |2026-04-16 17:30:30 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
470     |2026-04-16 16:21:23 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
469     |2026-04-16 15:54:57 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
468     |2026-04-16 15:39:05 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
467     |2026-04-16 15:38:20 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
466     |2026-04-16 11:09:05 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
465     |2026-04-16 11:08:54 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
464     |2026-04-16 11:05:52 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
463     |2026-04-16 11:01:01 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
462     |2026-04-16 10:14:09 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
461     |2026-04-16 10:14:01 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
460     |2026-04-16 09:47:20 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
459     |2026-04-16 09:44:37 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
458     |2026-04-15 14:06:58 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
457     |2026-04-15 14:06:36 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
456     |2026-04-15 13:41:08 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
455     |2026-04-15 13:41:07 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
454     |2026-04-15 13:40:43 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
453     |2026-04-15 13:39:56 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
452     |2026-04-15 13:29:25 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
451     |2026-04-15 13:29:21 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
450     |2026-04-15 13:28:59 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
449     |2026-04-15 13:27:43 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
448     |2026-04-15 13:08:44 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
447     |2026-04-15 13:07:59 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
446     |2026-04-15 12:57:17 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
445     |2026-04-15 12:57:16 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
444     |2026-04-15 12:56:42 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
443     |2026-04-15 12:56:07 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
442     |2026-04-15 12:49:38 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
441     |2026-04-15 12:49:34 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
440     |2026-04-15 12:49:11 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
439     |2026-04-15 12:48:52 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
438     |2026-04-15 12:08:58 |Minor       |0x08000004  |Deasserted  |The PCIe Card 6 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001030).
437     |2026-04-15 11:30:02 |Minor       |0x08000003  |Asserted    |The PCIe Card 6 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001030).
436     |2026-04-15 11:07:35 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
435     |2026-04-15 11:07:35 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
434     |2026-04-15 11:07:12 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
433     |2026-04-15 11:06:27 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
432     |2026-04-15 08:32:33 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
431     |2026-04-15 08:32:09 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
430     |2026-04-15 08:17:22 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
429     |2026-04-15 08:17:22 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
428     |2026-04-15 08:15:01 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
427     |2026-04-15 08:13:26 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
426     |2026-04-15 07:59:34 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
425     |2026-04-15 07:59:27 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
424     |2026-04-15 07:51:51 |Minor       |0x08000004  |Deasserted  |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
423     |2026-04-15 07:46:16 |Minor       |0x08000003  |Asserted    |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
422     |2026-04-15 07:43:17 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
421     |2026-04-15 07:41:49 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
420     |2026-04-15 07:26:39 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
419     |2026-04-15 07:26:38 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
418     |2026-04-15 07:22:45 |Minor       |0x08000004  |Deasserted  |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
417     |2026-04-15 07:08:33 |Minor       |0x08000003  |Asserted    |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
416     |2026-04-15 07:00:30 |Minor       |0x08000004  |Deasserted  |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
415     |2026-04-15 06:23:17 |Minor       |0x08000003  |Asserted    |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
414     |2026-04-15 06:20:05 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
413     |2026-04-15 06:15:39 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
412     |2026-04-15 04:49:17 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
411     |2026-04-15 04:44:15 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
410     |2026-04-15 04:38:36 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
409     |2026-04-15 04:07:38 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
408     |2026-04-15 03:44:05 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
407     |2026-04-15 03:39:12 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
406     |2026-04-15 03:38:08 |Minor       |0x08000004  |Deasserted  |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
405     |2026-04-15 03:36:07 |Minor       |0x08000003  |Asserted    |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
404     |2026-04-15 03:31:22 |Minor       |0x08000004  |Deasserted  |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
403     |2026-04-15 03:29:09 |Minor       |0x08000003  |Asserted    |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
402     |2026-04-15 03:28:01 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
401     |2026-04-15 03:25:55 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
400     |2026-04-14 14:57:58 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
399     |2026-04-14 14:57:58 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
398     |2026-04-14 14:54:55 |Minor       |0x08000004  |Deasserted  |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
397     |2026-04-14 14:43:41 |Minor       |0x08000003  |Asserted    |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
396     |2026-04-14 14:43:11 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
395     |2026-04-14 14:40:35 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
394     |2026-04-14 14:08:18 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
393     |2026-04-14 14:04:47 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
392     |2026-04-14 14:04:24 |Minor       |0x08000004  |Deasserted  |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
391     |2026-04-14 13:43:55 |Minor       |0x08000003  |Asserted    |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
390     |2026-04-14 13:37:41 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
389     |2026-04-14 13:32:12 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
388     |2026-04-14 13:19:02 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
387     |2026-04-14 13:18:16 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
386     |2026-04-14 11:16:40 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
385     |2026-04-14 11:15:54 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
384     |2026-04-14 09:27:02 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
383     |2026-04-14 09:24:43 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
382     |2026-04-14 09:16:12 |Minor       |0x08000004  |Deasserted  |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
381     |2026-04-14 09:11:33 |Minor       |0x08000003  |Asserted    |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
380     |2026-04-14 09:02:10 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
379     |2026-04-14 08:55:07 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
378     |2026-04-14 08:41:26 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
377     |2026-04-14 08:40:38 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
376     |2026-04-14 08:13:17 |Minor       |0x08000004  |Deasserted  |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
375     |2026-04-14 08:13:16 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
374     |2026-04-14 08:00:05 |Minor       |0x08000004  |Deasserted  |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
373     |2026-04-14 07:55:05 |Minor       |0x08000003  |Asserted    |The PCIe Card 8 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000093).
372     |2026-04-14 07:52:11 |Minor       |0x08000003  |Asserted    |The PCIe Card 7 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001855).
371     |2026-04-14 07:47:30 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
370     |2026-04-14 07:30:51 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
369     |2026-04-14 07:30:18 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
368     |2026-04-11 14:02:33 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
367     |2026-04-11 14:01:37 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
366     |2026-04-11 13:42:33 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
365     |2026-04-11 12:59:09 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
364     |2026-04-11 12:47:48 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
363     |2026-04-11 08:46:21 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
362     |2026-04-11 08:36:55 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
361     |2026-04-11 08:35:48 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
360     |2026-04-11 08:26:04 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
359     |2026-04-11 03:24:04 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
358     |2026-04-11 03:11:19 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
357     |2026-04-11 00:11:50 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
356     |2026-04-11 00:01:55 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
355     |2026-04-11 00:00:37 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
354     |2026-04-10 23:51:00 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
353     |2026-04-10 23:50:38 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
352     |2026-04-10 23:39:55 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
351     |2026-04-10 21:31:08 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
350     |2026-04-10 21:17:47 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
349     |2026-04-10 20:59:56 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
348     |2026-04-10 20:47:55 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
347     |2026-04-10 17:41:34 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
346     |2026-04-10 17:30:17 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
345     |2026-04-10 17:29:11 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
344     |2026-04-10 17:19:06 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
343     |2026-04-10 17:18:07 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
342     |2026-04-10 17:08:21 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
341     |2026-04-10 15:37:23 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
340     |2026-04-10 15:28:16 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
339     |2026-04-10 11:14:52 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
338     |2026-04-10 11:05:06 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
337     |2026-04-10 11:04:00 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
336     |2026-04-10 10:54:43 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
335     |2026-04-10 10:17:25 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
334     |2026-04-10 10:04:31 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
333     |2026-04-10 10:04:09 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
332     |2026-04-10 09:54:30 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
331     |2026-04-10 09:53:32 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
330     |2026-04-10 09:42:40 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
329     |2026-04-10 08:24:40 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
328     |2026-04-10 08:11:52 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
327     |2026-04-10 05:15:16 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
326     |2026-04-10 02:01:57 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
325     |2026-04-10 02:01:57 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
324     |2026-04-10 02:01:56 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
323     |2026-04-10 02:01:33 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
322     |2026-04-10 02:01:33 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
321     |2026-04-10 02:01:33 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
320     |2026-04-09 16:52:49 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
319     |2026-04-09 16:08:51 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
318     |2026-04-09 15:55:17 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
317     |2026-04-09 15:54:24 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
316     |2026-04-09 15:43:07 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
315     |2026-04-09 15:41:51 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
314     |2026-04-09 12:52:55 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
313     |2026-04-09 09:38:32 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
312     |2026-04-09 09:26:54 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
311     |2026-04-09 08:37:02 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
310     |2026-04-09 08:28:22 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
309     |2026-04-09 08:27:27 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
308     |2026-04-09 07:15:21 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (86 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
307     |2026-04-09 07:15:18 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
306     |2026-04-09 07:15:18 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
305     |2026-04-09 07:15:06 |Minor       |0x08000004  |Deasserted  |The PCIe Card 6 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001030).
304     |2026-04-09 07:14:55 |Minor       |0x08000003  |Asserted    |The PCIe Card 6 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001030).
303     |2026-04-09 07:14:47 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (86 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
302     |2026-04-09 07:14:43 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
301     |2026-04-09 07:14:43 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
300     |2026-04-09 07:13:16 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
299     |2026-04-09 07:13:13 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
298     |2026-04-09 07:13:12 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
297     |2026-04-09 07:12:39 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
296     |2026-04-09 07:12:28 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
295     |2026-04-09 07:12:19 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
294     |2026-04-09 07:12:07 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
293     |2026-04-09 07:12:05 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
292     |2026-04-09 07:11:42 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
291     |2026-04-09 07:11:22 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
290     |2026-04-09 07:10:50 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
289     |2026-04-09 07:10:45 |Minor       |0x08000004  |Deasserted  |The PCIe Card 6 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001030).
288     |2026-04-09 07:10:45 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
287     |2026-04-09 07:10:45 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
286     |2026-04-09 07:10:22 |Minor       |0x08000003  |Asserted    |The PCIe Card 6 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438001030).
285     |2026-04-09 07:10:11 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
284     |2026-04-09 07:10:11 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
283     |2026-04-09 07:10:06 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
282     |2026-04-09 07:09:04 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
281     |2026-04-09 07:09:03 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
280     |2026-04-09 07:09:00 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
279     |2026-04-09 07:08:42 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
278     |2026-04-09 07:08:41 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
277     |2026-04-09 07:08:28 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
276     |2026-04-09 07:07:44 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
275     |2026-04-09 07:07:19 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
274     |2026-04-09 07:06:44 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
273     |2026-04-09 07:06:44 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
272     |2026-04-09 07:06:35 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
271     |2026-04-09 07:06:01 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
270     |2026-04-09 07:05:59 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
269     |2026-04-09 07:05:58 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
268     |2026-04-09 07:05:37 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
267     |2026-04-09 07:05:34 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
266     |2026-04-09 07:05:12 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
265     |2026-04-09 07:04:53 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
264     |2026-04-09 07:04:31 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
263     |2026-04-09 07:04:27 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
262     |2026-04-09 07:04:08 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
261     |2026-04-09 07:04:04 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
260     |2026-04-09 07:03:23 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
259     |2026-04-09 07:03:20 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
258     |2026-04-09 07:03:12 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
257     |2026-04-09 07:02:50 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
256     |2026-04-09 07:02:50 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
255     |2026-04-09 07:02:46 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
254     |2026-04-09 07:02:17 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
253     |2026-04-09 07:02:17 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
252     |2026-04-09 07:02:12 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
251     |2026-04-09 07:01:43 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
250     |2026-04-09 07:01:43 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
249     |2026-04-09 07:01:37 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
248     |2026-04-09 07:00:36 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
247     |2026-04-09 07:00:29 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
246     |2026-04-09 07:00:14 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
245     |2026-04-09 07:00:06 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
244     |2026-04-09 06:59:10 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
243     |2026-04-09 06:59:08 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
242     |2026-04-09 06:59:08 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
241     |2026-04-09 06:58:59 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
240     |2026-04-09 06:58:35 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
239     |2026-04-09 06:58:34 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
238     |2026-04-09 06:58:00 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
237     |2026-04-09 06:57:50 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
236     |2026-04-09 06:57:39 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
235     |2026-04-09 06:57:39 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
234     |2026-04-09 06:56:22 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
233     |2026-04-09 06:55:49 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
232     |2026-04-09 06:45:51 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
231     |2026-04-09 06:45:28 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
230     |2026-04-09 06:45:06 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
229     |2026-04-09 06:45:05 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
228     |2026-04-09 06:44:42 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
227     |2026-04-09 06:44:31 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
226     |2026-04-09 06:43:57 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
225     |2026-04-09 06:43:24 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
224     |2026-04-09 06:42:49 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
223     |2026-04-09 06:42:13 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
222     |2026-04-09 06:30:14 |Normal      |0x1A00006F  |Asserted    |The openUBMC is reset, with the cause code of 0x2.
221     |2026-04-09 06:30:01 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
220     |2026-04-09 06:20:22 |Normal      |0x1A00006F  |Asserted    |The openUBMC is reset, with the cause code of 0x2.
219     |2026-04-09 06:20:05 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
218     |2026-04-09 04:05:52 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (90 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
217     |2026-04-09 04:01:43 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (90 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
216     |2026-04-09 03:52:27 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (99 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
215     |2026-04-09 03:51:54 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (99 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
214     |2026-04-09 03:48:02 |Major       |0x03000008  |Deasserted  |Lost power supply redundancy.
213     |2026-04-09 03:47:42 |Major       |0x03000007  |Asserted    |Lost power supply redundancy.
212     |2026-04-09 03:47:25 |Normal      |0x1A00006F  |Asserted    |The openUBMC is reset, with the cause code of 0x2.
211     |2026-04-09 03:46:39 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
210     |2026-04-09 03:33:54 |Normal      |0x1A00006F  |Asserted    |The openUBMC is reset, with the cause code of 0x2.
209     |2026-04-09 03:33:14 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
208     |2026-04-09 02:15:22 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
207     |2026-04-09 02:15:22 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
206     |2026-04-09 02:15:11 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
205     |2026-04-09 02:14:49 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
204     |2026-04-09 02:14:49 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
203     |2026-04-09 02:14:49 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
202     |2026-04-09 02:13:19 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
201     |2026-04-09 02:13:18 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
200     |2026-04-09 02:13:18 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
199     |2026-04-09 02:12:46 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
198     |2026-04-09 02:12:45 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
197     |2026-04-09 02:12:45 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
196     |2026-04-09 02:11:48 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
195     |2026-04-09 02:11:48 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
194     |2026-04-09 02:11:37 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
193     |2026-04-09 02:11:37 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
192     |2026-04-09 02:05:11 |Normal      |0x0800003F  |Asserted    |The PCIe card 12 (SP686C-M-16i 4G) BBU is present.
191     |2026-04-09 02:03:04 |Normal      |0x080000BD  |Asserted    |PCIe Card 4 (Mars X201) is replaced from SN(AENA2441002105) to SN(AENA2438000111) (SN:AENA2438000111).
190     |2026-04-09 02:03:04 |Normal      |0x080000BD  |Asserted    |PCIe Card 5 (Mars X201) is replaced from SN(AENA2438000111) to SN(AENA2441002105) (SN:AENA2441002105).
189     |2026-04-09 02:02:48 |Normal      |0x080000BD  |Asserted    |PCIe Card 3 (Mars X201) is replaced from SN(AENA24360003) to SN(AENA2436000348) (SN:AENA2436000348).
188     |2026-04-09 02:02:46 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-04-09 01:59:43 UTC, The power has been already restored.
187     |2026-04-09 02:00:17 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
186     |2026-04-09 02:00:15 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
185     |2026-04-09 01:59:54 |Normal      |0x1A00000D  |Asserted    |openUBMC is restarted after AC power supply is restored.
184     |2026-04-09 01:36:01 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
183     |2026-04-07 10:51:23 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
182     |2026-04-07 10:51:18 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
181     |2026-04-07 10:48:34 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
180     |2026-04-04 08:10:52 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
179     |2026-04-04 08:10:46 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
178     |2026-04-04 08:08:04 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
177     |2026-04-03 09:33:17 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
176     |2026-04-03 09:33:12 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
175     |2026-04-03 09:30:32 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
174     |2026-04-03 09:14:49 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
173     |2026-04-03 09:14:43 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
172     |2026-04-03 09:12:04 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
171     |2026-04-03 09:01:59 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
170     |2026-04-03 09:01:54 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
169     |2026-04-03 08:59:13 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
168     |2026-04-03 08:49:17 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
167     |2026-04-03 08:49:11 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
166     |2026-04-03 08:46:31 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
165     |2026-04-03 08:38:47 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
164     |2026-04-03 08:38:41 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
163     |2026-04-03 08:36:02 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
162     |2026-04-03 08:17:05 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
161     |2026-04-03 08:16:59 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
160     |2026-04-03 08:14:20 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
159     |2026-04-03 07:59:42 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
158     |2026-04-03 07:59:36 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
157     |2026-04-03 07:56:57 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
156     |2026-04-03 07:49:40 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
155     |2026-04-03 07:49:34 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
154     |2026-04-03 07:46:55 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
153     |2026-04-03 05:30:41 |Critical    |0x02000014  |Deasserted  |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
152     |2026-04-03 05:30:35 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
151     |2026-04-03 05:30:30 |Normal      |0x080000BD  |Asserted    |PCIe Card 3 (Mars X201) is replaced from SN(AENA2436000348) to SN(AENA24360003) (SN:AENA24360003).
150     |2026-04-03 05:27:52 |Critical    |0x02000013  |Asserted    |The disk Disk9 triggered an uncorrectable error, NA (SN:035AMGD9Q5000667).
149     |2026-04-03 03:54:14 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
148     |2026-04-03 03:48:37 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
147     |2026-04-03 03:30:43 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
146     |2026-04-03 01:58:14 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
145     |2026-04-03 01:58:04 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
144     |2026-04-03 01:47:18 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
143     |2026-04-03 01:46:45 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
142     |2026-04-02 23:18:37 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
141     |2026-04-02 23:03:05 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
140     |2026-04-02 22:26:21 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
139     |2026-04-02 21:21:12 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
138     |2026-04-02 20:57:34 |Minor       |0x08000004  |Deasserted  |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
137     |2026-04-02 19:21:52 |Minor       |0x08000003  |Asserted    |The PCIe Card 10 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2449000694).
136     |2026-04-02 17:14:11 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
135     |2026-04-02 16:50:33 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
134     |2026-04-02 16:43:09 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
133     |2026-04-02 16:04:12 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
132     |2026-04-02 15:53:31 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
131     |2026-04-02 15:53:09 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
130     |2026-04-02 15:42:27 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
129     |2026-04-02 15:41:33 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
128     |2026-04-02 15:33:25 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
127     |2026-04-02 15:32:52 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
126     |2026-04-02 15:22:31 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
125     |2026-04-02 15:12:34 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
124     |2026-04-02 14:49:20 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
123     |2026-04-02 13:52:09 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
122     |2026-04-02 13:43:14 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
121     |2026-04-02 13:06:11 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
120     |2026-04-02 12:57:08 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
119     |2026-04-02 12:56:24 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
118     |2026-04-02 12:47:51 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
117     |2026-04-02 12:21:34 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
116     |2026-04-02 12:04:33 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
115     |2026-04-02 12:04:10 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
114     |2026-04-02 11:52:42 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
113     |2026-04-02 11:52:20 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
112     |2026-04-02 11:41:15 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
111     |2026-04-02 09:58:14 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
110     |2026-04-02 09:31:32 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
109     |2026-04-02 09:18:57 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
108     |2026-04-02 08:15:57 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
107     |2026-04-02 08:15:35 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
106     |2026-04-02 07:47:28 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
105     |2026-04-02 07:47:16 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
104     |2026-04-02 07:40:36 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
103     |2026-04-02 07:40:36 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
102     |2026-04-02 07:40:14 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
101     |2026-04-02 07:40:14 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
100     |2026-04-02 07:36:42 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
99      |2026-04-02 07:36:20 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
98      |2026-04-02 07:32:59 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (84 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
97      |2026-04-02 07:32:37 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (84 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
96      |2026-04-02 07:29:38 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
95      |2026-04-02 07:29:27 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
94      |2026-04-02 07:25:57 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
93      |2026-04-02 07:25:23 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
92      |2026-04-02 06:53:09 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
91      |2026-04-02 06:52:47 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
90      |2026-04-02 06:44:37 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
89      |2026-04-02 06:44:26 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
88      |2026-04-02 06:42:35 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
87      |2026-04-02 06:42:24 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
86      |2026-04-02 06:12:57 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
85      |2026-04-02 06:12:23 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
84      |2026-04-02 06:05:32 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
83      |2026-04-02 06:04:59 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
82      |2026-04-02 05:15:21 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
81      |2026-04-02 05:14:58 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
80      |2026-04-02 05:11:38 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
79      |2026-04-02 05:11:27 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
78      |2026-04-02 05:11:05 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
77      |2026-04-02 05:10:54 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
76      |2026-04-02 05:07:56 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
75      |2026-04-02 05:07:34 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
74      |2026-04-02 05:07:23 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
73      |2026-04-02 05:07:23 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (81 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
72      |2026-04-02 04:59:47 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
71      |2026-04-02 04:59:46 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (85 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
70      |2026-04-02 04:59:46 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (84 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
69      |2026-04-02 04:59:35 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (84 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
68      |2026-04-02 04:59:24 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
67      |2026-04-02 04:59:24 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (85 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
66      |2026-04-02 04:57:33 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
65      |2026-04-02 04:57:11 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
64      |2026-04-02 04:56:59 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
63      |2026-04-02 04:56:49 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
62      |2026-04-02 04:55:31 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
61      |2026-04-02 04:55:07 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
60      |2026-04-02 04:54:56 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
59      |2026-04-02 04:54:46 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
58      |2026-04-02 04:51:46 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (84 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
57      |2026-04-02 04:51:36 |Minor       |0x08000004  |Deasserted  |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
56      |2026-04-02 04:51:25 |Minor       |0x08000004  |Deasserted  |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
55      |2026-04-02 04:51:13 |Minor       |0x08000003  |Asserted    |The PCIe Card 5 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2438000111).
54      |2026-04-02 04:51:02 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (84 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
53      |2026-04-02 04:51:02 |Minor       |0x08000003  |Asserted    |The PCIe Card 3 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2436000348).
52      |2026-04-02 04:49:44 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
51      |2026-04-02 04:49:22 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
50      |2026-04-02 04:45:38 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
49      |2026-04-02 04:45:05 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (83 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
48      |2026-04-02 04:40:26 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
47      |2026-04-02 04:40:04 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (82 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
46      |2026-04-02 04:07:03 |Minor       |0x08000004  |Deasserted  |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
45      |2026-04-02 04:06:52 |Minor       |0x08000003  |Asserted    |The PCIe Card 4 (Mars X201) temperature (80 degrees C) exceeds the overtemperature threshold (80 degrees C) (SN:AENA2441002105).
44      |2026-04-01 01:54:16 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-04-01 01:51:15 UTC, The power has been already restored.
43      |2026-04-01 01:51:53 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
42      |2026-04-01 01:51:50 |Normal      |0x1A00000D  |Asserted    |openUBMC is restarted after AC power supply is restored.
41      |2026-04-01 01:51:24 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
40      |2026-04-01 01:27:56 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
39      |2026-03-31 09:28:58 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
38      |2026-03-31 09:01:43 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
37      |2026-03-31 08:02:07 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
36      |2026-03-31 04:02:21 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-03-31 03:59:20 UTC, The power has been already restored.
35      |2026-03-31 03:59:57 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
34      |2026-03-31 03:59:57 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
33      |2026-03-31 03:59:24 |Normal      |0x1A00000D  |Asserted    |openUBMC is restarted after AC power supply is restored.
32      |2026-03-31 01:30:26 |Critical    |0x0300000D  |Asserted    |The AC/DC input of PSU 3 is lost or out-of-range (SN:1401202N0A254600420, BN:302003488).
31      |2026-03-31 01:30:19 |Critical    |0x0300000D  |Asserted    |The AC/DC input of PSU 4 is lost or out-of-range (SN:1401202N0A254600484, BN:302003488).
30      |2026-03-31 01:28:28 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
29      |2026-03-11 07:50:38 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
28      |2026-03-11 07:28:17 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
27      |2026-03-11 07:22:35 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
26      |2026-03-06 06:41:37 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
25      |2026-03-06 06:19:37 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
24      |2026-02-28 15:21:52 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
23      |2026-02-28 14:50:10 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
22      |2026-02-10 10:52:45 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
21      |2026-02-10 10:49:48 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
20      |2026-02-10 10:22:04 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
19      |2026-02-10 09:40:58 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
18      |2026-02-05 12:02:51 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
17      |2026-02-05 11:52:32 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
16      |2026-02-05 11:36:20 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-02-05 11:33:20 UTC, The power has been already restored.
15      |2026-02-05 11:33:17 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
14      |2026-02-05 11:33:16 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
13      |2026-02-05 11:32:51 |Normal      |0x1A00000D  |Asserted    |openUBMC is restarted after AC power supply is restored.
12      |2026-02-05 11:00:42 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
11      |2026-02-04 09:23:17 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
10      |2026-02-04 08:54:42 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
9       |2026-02-04 08:54:27 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-02-04 08:51:27 UTC, The power has been already restored.
8       |2026-02-04 08:52:04 |Critical    |0x0300000D  |Asserted    |The AC/DC input of PSU 1 is lost or out-of-range (SN:1401202N0A254600411, BN:302003488).
7       |2026-02-04 08:52:04 |Critical    |0x0300000D  |Asserted    |The AC/DC input of PSU 3 is lost or out-of-range (SN:1401202N0A254600420, BN:302003488).
6       |2026-02-04 08:52:04 |Critical    |0x0300000D  |Asserted    |The AC/DC input of PSU 2 is lost or out-of-range (SN:1401202N0A254600447, BN:302003488).
5       |2026-02-04 08:50:48 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
4       |2026-02-04 08:50:41 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
3       |2026-02-04 08:50:16 |Normal      |0x1A00000D  |Asserted    |openUBMC is restarted after AC power supply is restored.
2       |2026-01-28 02:55:10 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
1       |2026-01-28 02:54:48 |Normal      |0x1A00000F  |Asserted    |openUBMC event records are cleared.
