
Fan:| Fan_3_010103:
--| FanObjectName:       Fan_3_010103
--| IdentifyStatus:       2
--| SingleConnector:
--| DualConnector:
--| PowerGood:       1
--| MaxSupportedPWM:       255
--| DeviceName:       
--| FunctionDesc:       
--| SpeedStable:       true
--| FanId:       3
--| SystemId:       1
--| RearMaxSpeed:       15000
--| FrontMaxSpeed:       15000
--| PartNumber:       02314BLG
--| RearRPM:       0
--| FrontRPM:       0
--| RearStatus:       0
--| FrontStatus:       0
--| RearSpeed:       4096
--| FrontSpeed:       0
--| RearPresence:       1
--| FrontPresence:       1
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| Model:       02314BLG 8038+
--| IsTwins:       false
--| Type:       0
--| Slot:       3
--| IdentifySpeedLevel:       35
--| Position:       CLU1
--| BOM:       BOM32030275
--| FanAlarmLed:       0
--| ExpectedPWM:       89
--| PWMPercentage:       34
--| HardwarePWM:       89
--| ObjectName:       Fan_3_010103
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010103
--| ClassName:       Fan
--| last_present:       1
--| model_source:       3
--| default_model:       02314BLG 8038+
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       3
| Fan_4_010103:
--| FanObjectName:       Fan_4_010103
--| IdentifyStatus:       2
--| SingleConnector:
--| DualConnector:
--| PowerGood:       1
--| MaxSupportedPWM:       255
--| DeviceName:       
--| FunctionDesc:       
--| SpeedStable:       true
--| FanId:       4
--| SystemId:       1
--| RearMaxSpeed:       15000
--| FrontMaxSpeed:       15000
--| PartNumber:       02314BLG
--| RearRPM:       0
--| FrontRPM:       0
--| RearStatus:       0
--| FrontStatus:       0
--| RearSpeed:       4096
--| FrontSpeed:       0
--| RearPresence:       1
--| FrontPresence:       1
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| Model:       02314BLG 8038+
--| IsTwins:       false
--| Type:       0
--| Slot:       4
--| IdentifySpeedLevel:       35
--| Position:       CLU1
--| BOM:       BOM32030275
--| FanAlarmLed:       0
--| ExpectedPWM:       89
--| PWMPercentage:       34
--| HardwarePWM:       89
--| ObjectName:       Fan_4_010103
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010103
--| ClassName:       Fan
--| last_present:       1
--| model_source:       3
--| default_model:       02314BLG 8038+
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       4
| Fan_1_010103:
--| FanObjectName:       Fan_1_010103
--| IdentifyStatus:       2
--| SingleConnector:
--| DualConnector:
--| PowerGood:       1
--| MaxSupportedPWM:       255
--| DeviceName:       
--| FunctionDesc:       
--| SpeedStable:       true
--| FanId:       1
--| SystemId:       1
--| RearMaxSpeed:       15000
--| FrontMaxSpeed:       15000
--| PartNumber:       02314BLG
--| RearRPM:       0
--| FrontRPM:       0
--| RearStatus:       0
--| FrontStatus:       0
--| RearSpeed:       4096
--| FrontSpeed:       0
--| RearPresence:       1
--| FrontPresence:       1
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| Model:       02314BLG 8038+
--| IsTwins:       false
--| Type:       0
--| Slot:       1
--| IdentifySpeedLevel:       35
--| Position:       CLU1
--| BOM:       BOM32030275
--| FanAlarmLed:       0
--| ExpectedPWM:       89
--| PWMPercentage:       34
--| HardwarePWM:       89
--| ObjectName:       Fan_1_010103
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010103
--| ClassName:       Fan
--| last_present:       1
--| model_source:       3
--| default_model:       02314BLG 8038+
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       1
| Fan_2_010103:
--| FanObjectName:       Fan_2_010103
--| IdentifyStatus:       2
--| SingleConnector:
--| DualConnector:
--| PowerGood:       1
--| MaxSupportedPWM:       255
--| DeviceName:       
--| FunctionDesc:       
--| SpeedStable:       true
--| FanId:       2
--| SystemId:       1
--| RearMaxSpeed:       15000
--| FrontMaxSpeed:       15000
--| PartNumber:       02314BLG
--| RearRPM:       0
--| FrontRPM:       0
--| RearStatus:       0
--| FrontStatus:       0
--| RearSpeed:       4096
--| FrontSpeed:       0
--| RearPresence:       1
--| FrontPresence:       1
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| Model:       02314BLG 8038+
--| IsTwins:       false
--| Type:       0
--| Slot:       2
--| IdentifySpeedLevel:       35
--| Position:       CLU1
--| BOM:       BOM32030275
--| FanAlarmLed:       0
--| ExpectedPWM:       89
--| PWMPercentage:       34
--| HardwarePWM:       89
--| ObjectName:       Fan_2_010103
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010103
--| ClassName:       Fan
--| last_present:       1
--| model_source:       3
--| default_model:       02314BLG 8038+
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       2

FanType:| FanType_8080P_010103:
--| FanTypeObjectName:       FanType_8080P_010103
--| SystemId:       1
--| FanDiameterMm:       80
--| PowerRange:
----| 1:       120
----| 2:       120
----| 3:       190
----| 4:       390
----| 5:       680
----| 6:       1050
----| 7:       1800
----| 8:       2400
----| 9:       3600
----| 10:       5200
--| SpeedRange:
----| 1:       0
----| 2:       20
----| 3:       30
----| 4:       40
----| 5:       50
----| 6:       60
----| 7:       70
----| 8:       80
----| 9:       90
----| 10:       100
--| IsTwins:       true
--| IdentifyRangeHigh:       6641
--| IdentifyRangeLow:       4908
--| IsDefaultType:       true
--| Index:       2
--| MatchedCount:       0
--| PartNumber:       02314EWC
--| BOM:       BOM32030389-001
--| RearMaxSpeed:       16500
--| Name:       02314EWC 8080+
--| FrontMaxSpeed:       16500
--| ObjectName:       FanType_8080P_010103
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010103
--| ClassName:       FanType
--| fan_num:       0
| FanType_8038P_010103:
--| FanTypeObjectName:       FanType_8038P_010103
--| SystemId:       1
--| FanDiameterMm:       80
--| PowerRange:
----| 1:       120
----| 2:       120
----| 3:       190
----| 4:       390
----| 5:       680
----| 6:       1050
----| 7:       1800
----| 8:       2400
----| 9:       3600
----| 10:       5200
--| SpeedRange:
----| 1:       0
----| 2:       20
----| 3:       30
----| 4:       40
----| 5:       50
----| 6:       60
----| 7:       70
----| 8:       80
----| 9:       90
----| 10:       100
--| IsTwins:       false
--| IdentifyRangeHigh:       4750
--| IdentifyRangeLow:       3230
--| IsDefaultType:       true
--| Index:       1
--| MatchedCount:       0
--| PartNumber:       02314BLG
--| BOM:       BOM32030275
--| RearMaxSpeed:       15000
--| Name:       02314BLG 8038+
--| FrontMaxSpeed:       15000
--| ObjectName:       FanType_8038P_010103
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010103
--| ClassName:       FanType
--| fan_num:       4



