
Fan:| Fan_2_010106:
--| DualConnector:
--| FanObjectName:       Fan_2_010106
--| SingleConnector:
--| PowerGood:       1
--| IdentifyStatus:       2
--| Type:       0
--| RearStatus:       0
--| Slot:       2
--| SpeedStable:       true
--| FrontPresence:       1
--| FrontSpeed:       4440
--| FrontStatus:       0
--| HardwarePWM:       68
--| FanId:       2
--| SystemId:       1
--| MaxSupportedPWM:       255
--| BOM:       BOM31167289
--| FrontMaxSpeed:       16500
--| IsTwins:       true
--| RearMaxSpeed:       16500
--| IdentifySpeedLevel:       50
--| FanAlarmLed:       0
--| PWMPercentage:       26
--| RearSpeed:       4440
--| RearRPM:       0
--| FrontRPM:       0
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| RearPresence:       1
--| DeviceName:       
--| ExpectedPWM:       68
--| Model:       31167289 8080
--| PartNumber:       31167289
--| FunctionDesc:       
--| Position:       CLU
--| ObjectName:       Fan_2_010106
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010106
--| ClassName:       Fan
--| last_present:       1
--| model_source:       1
--| default_model:       31167289 8080
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       2
| Fan_6_010106:
--| DualConnector:
--| FanObjectName:       Fan_6_010106
--| SingleConnector:
--| PowerGood:       1
--| IdentifyStatus:       2
--| Type:       0
--| RearStatus:       0
--| Slot:       6
--| SpeedStable:       true
--| FrontPresence:       1
--| FrontSpeed:       4440
--| FrontStatus:       0
--| HardwarePWM:       68
--| FanId:       6
--| SystemId:       1
--| MaxSupportedPWM:       255
--| BOM:       BOM31167289
--| FrontMaxSpeed:       16500
--| IsTwins:       true
--| RearMaxSpeed:       16500
--| IdentifySpeedLevel:       50
--| FanAlarmLed:       0
--| PWMPercentage:       26
--| RearSpeed:       4440
--| RearRPM:       0
--| FrontRPM:       0
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| RearPresence:       1
--| DeviceName:       
--| ExpectedPWM:       68
--| Model:       31167289 8080
--| PartNumber:       31167289
--| FunctionDesc:       
--| Position:       CLU
--| ObjectName:       Fan_6_010106
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010106
--| ClassName:       Fan
--| last_present:       1
--| model_source:       1
--| default_model:       31167289 8080
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       6
| Fan_8_010106:
--| DualConnector:
--| FanObjectName:       Fan_8_010106
--| SingleConnector:
--| PowerGood:       1
--| IdentifyStatus:       2
--| Type:       0
--| RearStatus:       0
--| Slot:       8
--| SpeedStable:       true
--| FrontPresence:       1
--| FrontSpeed:       4440
--| FrontStatus:       0
--| HardwarePWM:       68
--| FanId:       8
--| SystemId:       1
--| MaxSupportedPWM:       255
--| BOM:       BOM31167289
--| FrontMaxSpeed:       16500
--| IsTwins:       true
--| RearMaxSpeed:       16500
--| IdentifySpeedLevel:       50
--| FanAlarmLed:       0
--| PWMPercentage:       26
--| RearSpeed:       4440
--| RearRPM:       0
--| FrontRPM:       0
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| RearPresence:       1
--| DeviceName:       
--| ExpectedPWM:       68
--| Model:       31167289 8080
--| PartNumber:       31167289
--| FunctionDesc:       
--| Position:       CLU
--| ObjectName:       Fan_8_010106
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010106
--| ClassName:       Fan
--| last_present:       1
--| model_source:       1
--| default_model:       31167289 8080
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       8
| Fan_1_010106:
--| DualConnector:
--| FanObjectName:       Fan_1_010106
--| SingleConnector:
--| PowerGood:       1
--| IdentifyStatus:       2
--| Type:       0
--| RearStatus:       0
--| Slot:       1
--| SpeedStable:       true
--| FrontPresence:       1
--| FrontSpeed:       6660
--| FrontStatus:       0
--| HardwarePWM:       102
--| FanId:       1
--| SystemId:       1
--| MaxSupportedPWM:       255
--| BOM:       BOM31167289
--| FrontMaxSpeed:       16500
--| IsTwins:       true
--| RearMaxSpeed:       16500
--| IdentifySpeedLevel:       50
--| FanAlarmLed:       0
--| PWMPercentage:       40
--| RearSpeed:       6720
--| RearRPM:       0
--| FrontRPM:       0
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| RearPresence:       1
--| DeviceName:       
--| ExpectedPWM:       102
--| Model:       31167289 8080
--| PartNumber:       31167289
--| FunctionDesc:       
--| Position:       CLU
--| ObjectName:       Fan_1_010106
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010106
--| ClassName:       Fan
--| last_present:       1
--| model_source:       1
--| default_model:       31167289 8080
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       1
| Fan_4_010106:
--| DualConnector:
--| FanObjectName:       Fan_4_010106
--| SingleConnector:
--| PowerGood:       1
--| IdentifyStatus:       2
--| Type:       0
--| RearStatus:       0
--| Slot:       4
--| SpeedStable:       true
--| FrontPresence:       1
--| FrontSpeed:       4440
--| FrontStatus:       0
--| HardwarePWM:       68
--| FanId:       4
--| SystemId:       1
--| MaxSupportedPWM:       255
--| BOM:       BOM31167289
--| FrontMaxSpeed:       16500
--| IsTwins:       true
--| RearMaxSpeed:       16500
--| IdentifySpeedLevel:       50
--| FanAlarmLed:       0
--| PWMPercentage:       26
--| RearSpeed:       4440
--| RearRPM:       0
--| FrontRPM:       0
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| RearPresence:       1
--| DeviceName:       
--| ExpectedPWM:       68
--| Model:       31167289 8080
--| PartNumber:       31167289
--| FunctionDesc:       
--| Position:       CLU
--| ObjectName:       Fan_4_010106
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010106
--| ClassName:       Fan
--| last_present:       1
--| model_source:       1
--| default_model:       31167289 8080
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       4
| Fan_3_010106:
--| DualConnector:
--| FanObjectName:       Fan_3_010106
--| SingleConnector:
--| PowerGood:       1
--| IdentifyStatus:       2
--| Type:       0
--| RearStatus:       0
--| Slot:       3
--| SpeedStable:       true
--| FrontPresence:       1
--| FrontSpeed:       6660
--| FrontStatus:       0
--| HardwarePWM:       102
--| FanId:       3
--| SystemId:       1
--| MaxSupportedPWM:       255
--| BOM:       BOM31167289
--| FrontMaxSpeed:       16500
--| IsTwins:       true
--| RearMaxSpeed:       16500
--| IdentifySpeedLevel:       50
--| FanAlarmLed:       0
--| PWMPercentage:       40
--| RearSpeed:       6660
--| RearRPM:       0
--| FrontRPM:       0
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| RearPresence:       1
--| DeviceName:       
--| ExpectedPWM:       102
--| Model:       31167289 8080
--| PartNumber:       31167289
--| FunctionDesc:       
--| Position:       CLU
--| ObjectName:       Fan_3_010106
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010106
--| ClassName:       Fan
--| last_present:       1
--| model_source:       1
--| default_model:       31167289 8080
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       3
| Fan_5_010106:
--| DualConnector:
--| FanObjectName:       Fan_5_010106
--| SingleConnector:
--| PowerGood:       1
--| IdentifyStatus:       2
--| Type:       0
--| RearStatus:       0
--| Slot:       5
--| SpeedStable:       true
--| FrontPresence:       1
--| FrontSpeed:       6720
--| FrontStatus:       0
--| HardwarePWM:       102
--| FanId:       5
--| SystemId:       1
--| MaxSupportedPWM:       255
--| BOM:       BOM31167289
--| FrontMaxSpeed:       16500
--| IsTwins:       true
--| RearMaxSpeed:       16500
--| IdentifySpeedLevel:       50
--| FanAlarmLed:       0
--| PWMPercentage:       40
--| RearSpeed:       6660
--| RearRPM:       0
--| FrontRPM:       0
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| RearPresence:       1
--| DeviceName:       
--| ExpectedPWM:       102
--| Model:       31167289 8080
--| PartNumber:       31167289
--| FunctionDesc:       
--| Position:       CLU
--| ObjectName:       Fan_5_010106
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010106
--| ClassName:       Fan
--| last_present:       1
--| model_source:       1
--| default_model:       31167289 8080
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       5
| Fan_7_010106:
--| DualConnector:
--| FanObjectName:       Fan_7_010106
--| SingleConnector:
--| PowerGood:       1
--| IdentifyStatus:       2
--| Type:       0
--| RearStatus:       0
--| Slot:       7
--| SpeedStable:       true
--| FrontPresence:       1
--| FrontSpeed:       6720
--| FrontStatus:       0
--| HardwarePWM:       102
--| FanId:       7
--| SystemId:       1
--| MaxSupportedPWM:       255
--| BOM:       BOM31167289
--| FrontMaxSpeed:       16500
--| IsTwins:       true
--| RearMaxSpeed:       16500
--| IdentifySpeedLevel:       50
--| FanAlarmLed:       0
--| PWMPercentage:       40
--| RearSpeed:       6660
--| RearRPM:       0
--| FrontRPM:       0
--| FanEntity:       
--| FanHealth:       0
--| Coefficient:       1
--| RearPresence:       1
--| DeviceName:       
--| ExpectedPWM:       102
--| Model:       31167289 8080
--| PartNumber:       31167289
--| FunctionDesc:       
--| Position:       CLU
--| ObjectName:       Fan_7_010106
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010106
--| ClassName:       Fan
--| last_present:       1
--| model_source:       1
--| default_model:       31167289 8080
--| mcu_upgrading:       false
--| status_record:
----| rear_error_count:       0
----| front_error_count:       0
--| status_error:
----| rear_error:       0
----| front_error:       0
--| persist_fan_id:       7

FanType:| FanType_8038P_010106:
--| FanTypeObjectName:       FanType_8038P_010106
--| SystemId:       1
--| IsDefaultType:       true
--| Index:       1
--| PartNumber:       02314BLG
--| Name:       02314BLG 8038+
--| FanDiameterMm:       80
--| PowerRange:
----| 1:       120
----| 2:       120
----| 3:       190
----| 4:       390
----| 5:       680
----| 6:       1050
----| 7:       1800
----| 8:       2400
----| 9:       3600
----| 10:       5200
--| SpeedRange:
----| 1:       0
----| 2:       20
----| 3:       30
----| 4:       40
----| 5:       50
----| 6:       60
----| 7:       70
----| 8:       80
----| 9:       90
----| 10:       100
--| MatchedCount:       0
--| IdentifyRangeHigh:       4750
--| IdentifyRangeLow:       3230
--| BOM:       BOM32030275
--| FrontMaxSpeed:       15000
--| IsTwins:       false
--| RearMaxSpeed:       15000
--| ObjectName:       FanType_8038P_010106
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010106
--| ClassName:       FanType
--| fan_num:       0
| FanType_8080P_010106:
--| FanTypeObjectName:       FanType_8080P_010106
--| SystemId:       1
--| IsDefaultType:       true
--| Index:       2
--| PartNumber:       31167289
--| Name:       31167289 8080
--| FanDiameterMm:       80
--| PowerRange:
----| 1:       120
----| 2:       120
----| 3:       190
----| 4:       390
----| 5:       680
----| 6:       1050
----| 7:       1800
----| 8:       2400
----| 9:       3600
----| 10:       5200
--| SpeedRange:
----| 1:       0
----| 2:       20
----| 3:       30
----| 4:       40
----| 5:       50
----| 6:       60
----| 7:       70
----| 8:       80
----| 9:       90
----| 10:       100
--| MatchedCount:       0
--| IdentifyRangeHigh:       9075
--| IdentifyRangeLow:       7425
--| BOM:       BOM31167289
--| FrontMaxSpeed:       16500
--| IsTwins:       true
--| RearMaxSpeed:       16500
--| ObjectName:       FanType_8080P_010106
--| ObjectIdentifier:
----| 1:       1
----| 2:       1
----| 3:       1
----| 4:       010106
--| ClassName:       FanType
--| fan_num:       8



