ID      |Generation Time     |Severity    |Event Code  |Status      |Event Description
746     |2026-08-17 12:53:53 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
745     |2026-08-17 12:53:51 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
744     |2026-08-17 12:53:46 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
743     |2026-08-17 12:53:44 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
742     |2026-08-17 12:53:41 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
741     |2026-08-17 12:53:38 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
740     |2026-08-17 12:53:32 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
739     |2026-08-17 12:53:30 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
738     |2026-08-17 12:53:01 |Normal      |0x1A000029  |Asserted    |BMC time is stepped by more than 10 minutes.
737     |2026-08-17 12:51:09 |Minor       |0x1A000055  |Asserted    |Failed to access the Self-description Record of PCIeRiser3 UBInterfaceCard8.
736     |2026-08-17 12:44:03 |Normal      |0x1A000029  |Asserted    |BMC time is stepped by more than 2 minutes.
735     |2026-08-17 12:31:49 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x10.
734     |2026-08-17 12:24:53 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
733     |2026-08-17 12:04:48 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
732     |2026-08-17 12:02:38 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x10.
731     |2026-08-17 11:42:19 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x10.
730     |2026-08-17 11:24:23 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x10.
729     |2026-08-17 11:24:12 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
728     |2026-08-17 11:15:07 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
727     |2026-08-17 09:57:47 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
726     |2026-08-17 09:55:58 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-08-17 09:32:11 UTC, The power has been already restored.
725     |2026-08-17 09:55:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
724     |2026-08-17 09:55:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
723     |2026-08-17 09:55:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
722     |2026-08-17 09:55:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
721     |2026-08-17 09:55:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
720     |2026-08-17 09:55:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
719     |2026-08-17 09:55:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
718     |2026-08-17 09:55:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
717     |2026-08-17 09:54:26 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
716     |2026-08-17 09:54:24 |Critical    |0x0300000D  |Asserted    |The AC/DC input of PSU 1 is lost or out-of-range (SN:2102312YKRJVRA038523, BN:02312YKR).
715     |2026-08-17 09:54:22 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
714     |2026-08-17 09:53:57 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
713     |2026-08-17 09:31:10 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
712     |2026-08-17 09:28:53 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-08-17 09:06:00 UTC, The power has been already restored.
711     |2026-08-17 09:28:17 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
710     |2026-08-17 09:28:17 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
709     |2026-08-17 09:28:17 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
708     |2026-08-17 09:28:17 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
707     |2026-08-17 09:28:16 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
706     |2026-08-17 09:28:16 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
705     |2026-08-17 09:28:16 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
704     |2026-08-17 09:28:16 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
703     |2026-08-17 09:27:20 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
702     |2026-08-17 09:27:08 |Critical    |0x0300000D  |Asserted    |The AC/DC input of PSU 1 is lost or out-of-range (SN:2102312YKRJVRA038523, BN:02312YKR).
701     |2026-08-17 09:27:05 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
700     |2026-08-17 09:26:46 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
699     |2026-08-15 11:24:57 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
698     |2026-08-15 11:12:01 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
697     |2026-08-15 11:12:01 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
696     |2026-08-15 11:12:00 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
695     |2026-08-15 11:12:00 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
694     |2026-08-15 11:12:00 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
693     |2026-08-15 11:12:00 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
692     |2026-08-15 11:11:24 |Normal      |0x02000023  |Asserted    |The disk Disk3 is replaced from SN(SH234506684) to SN(SH234502800) (SN:SH234502800).
691     |2026-08-15 11:11:24 |Normal      |0x02000023  |Asserted    |The disk Disk2 is replaced from SN(SH234502813) to SN(SH234506507) (SN:SH234506507).
690     |2026-08-15 11:11:24 |Normal      |0x02000023  |Asserted    |The disk Disk1 is replaced from SN(SH225102488) to SN(SH234506674) (SN:SH234506674).
689     |2026-08-15 11:11:24 |Normal      |0x02000023  |Asserted    |The disk Disk6 is replaced from SN(SH234502428) to SN(SH234506558) (SN:SH234506558).
688     |2026-08-15 11:11:23 |Normal      |0x02000023  |Asserted    |The disk Disk5 is replaced from SN(SH234503215) to SN(SH234506714) (SN:SH234506714).
687     |2026-08-15 11:11:23 |Normal      |0x02000023  |Asserted    |The disk Disk4 is replaced from SN(SH234505492) to SN(SH234502889) (SN:SH234502889).
686     |2026-08-15 11:11:23 |Normal      |0x02000023  |Asserted    |The disk Disk0 is replaced from SN(S6KNNT0Y911731) to SN(SH231801279) (SN:SH231801279).
685     |2026-08-15 11:11:08 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
684     |2026-08-15 11:10:44 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
683     |2026-08-15 11:10:27 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
682     |2026-08-15 05:13:10 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
681     |2026-08-15 05:09:40 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
680     |2026-08-15 05:06:11 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
679     |2026-08-15 05:02:42 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
678     |2026-08-15 04:59:11 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
677     |2026-08-15 04:55:41 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
676     |2026-08-15 04:52:11 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
675     |2026-08-15 04:48:42 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
674     |2026-08-15 04:45:12 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
673     |2026-08-15 04:41:42 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
672     |2026-08-15 04:38:12 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
671     |2026-08-15 04:34:43 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
670     |2026-08-15 04:31:13 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
669     |2026-08-15 04:27:38 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
668     |2026-08-15 04:24:08 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
667     |2026-08-15 04:20:38 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
666     |2026-08-15 04:17:12 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
665     |2026-08-15 04:13:39 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
664     |2026-08-15 04:10:10 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
663     |2026-08-15 04:06:40 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
662     |2026-08-15 04:03:10 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
661     |2026-08-15 03:59:39 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
660     |2026-08-15 03:56:09 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
659     |2026-08-15 03:52:40 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
658     |2026-08-15 03:49:09 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
657     |2026-08-15 03:45:38 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
656     |2026-08-15 03:42:08 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
655     |2026-08-15 03:38:39 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
654     |2026-08-15 03:35:09 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
653     |2026-08-15 03:31:40 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
652     |2026-08-15 03:28:10 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
651     |2026-08-15 03:24:40 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
650     |2026-08-15 03:21:09 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
649     |2026-08-15 03:17:40 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
648     |2026-08-15 03:14:11 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
647     |2026-08-15 03:10:35 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
646     |2026-08-15 03:07:05 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
645     |2026-08-15 03:03:34 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
644     |2026-08-15 03:00:05 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
643     |2026-08-15 02:56:35 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
642     |2026-08-15 02:53:05 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
641     |2026-08-15 02:49:34 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
640     |2026-08-15 02:46:04 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
639     |2026-08-15 02:42:34 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
638     |2026-08-15 02:38:59 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
637     |2026-08-15 02:35:29 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
636     |2026-08-15 02:32:03 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
635     |2026-08-15 02:28:29 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
634     |2026-08-15 02:24:59 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
633     |2026-08-15 02:21:27 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
632     |2026-08-15 02:17:57 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
631     |2026-08-15 02:14:27 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
630     |2026-08-15 02:10:58 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
629     |2026-08-15 02:07:28 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
628     |2026-08-15 02:03:57 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
627     |2026-08-15 02:00:27 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
626     |2026-08-15 01:56:57 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
625     |2026-08-15 01:53:27 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
624     |2026-08-15 01:49:55 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
623     |2026-08-15 01:46:25 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
622     |2026-08-15 01:42:56 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
621     |2026-08-15 01:39:28 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
620     |2026-08-15 01:35:56 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
619     |2026-08-15 01:32:25 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
618     |2026-08-15 01:28:55 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
617     |2026-08-15 01:25:30 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
616     |2026-08-15 01:21:56 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
615     |2026-08-15 01:18:25 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
614     |2026-08-15 01:14:54 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
613     |2026-08-15 01:11:20 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
612     |2026-08-15 01:07:50 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
611     |2026-08-15 01:04:21 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
610     |2026-08-15 01:00:51 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
609     |2026-08-15 00:57:22 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
608     |2026-08-15 00:53:52 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
607     |2026-08-15 00:50:22 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
606     |2026-08-15 00:46:52 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
605     |2026-08-15 00:43:20 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
604     |2026-08-15 00:39:51 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
603     |2026-08-15 00:36:20 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
602     |2026-08-15 00:32:55 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
601     |2026-08-15 00:29:21 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
600     |2026-08-15 00:25:51 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
599     |2026-08-15 00:22:21 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
598     |2026-08-15 00:18:52 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
597     |2026-08-15 00:15:17 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
596     |2026-08-15 00:11:47 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
595     |2026-08-15 00:08:17 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
594     |2026-08-15 00:04:48 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
593     |2026-08-15 00:01:18 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
592     |2026-08-14 23:57:48 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
591     |2026-08-14 23:54:18 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
590     |2026-08-14 23:50:48 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
589     |2026-08-14 23:47:19 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
588     |2026-08-14 23:43:48 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
587     |2026-08-14 23:40:18 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
586     |2026-08-14 23:36:47 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
585     |2026-08-14 23:33:17 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
584     |2026-08-14 23:29:48 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
583     |2026-08-14 23:26:21 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
582     |2026-08-14 22:50:23 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
581     |2026-08-14 22:39:55 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
580     |2026-08-14 22:33:15 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
579     |2026-08-14 22:28:09 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
578     |2026-08-14 22:28:08 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
577     |2026-08-14 22:25:28 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
576     |2026-08-14 20:41:08 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
575     |2026-08-14 20:41:06 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
574     |2026-08-14 20:39:42 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
573     |2026-08-14 20:11:00 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
572     |2026-08-14 20:05:57 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
571     |2026-08-14 20:05:56 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
570     |2026-08-14 20:03:26 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
569     |2026-08-14 19:19:26 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
568     |2026-08-14 19:19:25 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
567     |2026-08-14 19:15:42 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
566     |2026-08-14 18:58:45 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
565     |2026-08-14 18:58:44 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
564     |2026-08-14 18:54:46 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
563     |2026-08-14 17:22:40 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
562     |2026-08-14 17:22:40 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
561     |2026-08-14 17:22:40 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
560     |2026-08-14 17:22:39 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
559     |2026-08-14 17:22:39 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
558     |2026-08-14 17:22:39 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
557     |2026-08-14 17:21:41 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
556     |2026-08-14 17:21:34 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
555     |2026-08-14 17:21:34 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
554     |2026-08-14 17:21:34 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
553     |2026-08-14 17:21:33 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
552     |2026-08-14 17:21:32 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
551     |2026-08-14 17:21:32 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
550     |2026-08-14 17:21:30 |Major       |0x2C000008  |Deasserted  |The BC85ETHA power STBY_2V5_POWER failure results abnormal power-off.
549     |2026-08-14 17:20:32 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
548     |2026-08-14 17:17:24 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
547     |2026-08-14 17:17:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
546     |2026-08-14 17:17:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
545     |2026-08-14 17:17:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
544     |2026-08-14 17:17:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
543     |2026-08-14 17:17:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
542     |2026-08-14 17:16:22 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
541     |2026-08-14 17:16:18 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
540     |2026-08-14 17:16:17 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
539     |2026-08-14 17:16:17 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
538     |2026-08-14 17:16:16 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
537     |2026-08-14 17:16:15 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
536     |2026-08-14 17:16:14 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
535     |2026-08-14 17:16:13 |Major       |0x2C000007  |Asserted    |The BC85ETHA power STBY_2V5_POWER failure results abnormal power-off.
534     |2026-08-14 17:15:17 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
533     |2026-08-14 15:51:12 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
532     |2026-08-14 15:44:45 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
531     |2026-08-14 15:44:41 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
530     |2026-08-14 15:43:29 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
529     |2026-08-14 15:43:25 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
528     |2026-08-14 15:16:07 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
527     |2026-08-14 15:16:06 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
526     |2026-08-14 15:15:54 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
525     |2026-08-14 15:10:20 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
524     |2026-08-14 15:07:46 |Normal      |0x02000023  |Asserted    |The disk Disk0 is replaced from SN(SH234506595) to SN(S6KNNT0Y911731) (SN:S6KNNT0Y911731).
523     |2026-08-14 15:05:28 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
522     |2026-08-14 14:49:28 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
521     |2026-08-14 14:44:24 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
520     |2026-08-14 14:44:22 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
519     |2026-08-14 14:41:38 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
518     |2026-08-13 20:32:41 |Minor       |0x1A000055  |Asserted    |Failed to access the Self-description Record of PCIeRiser3 UBInterfaceCard7.
517     |2026-08-13 20:30:48 |Normal      |0x0100000F  |Asserted    |DIMM1B0 installed (SN:80CE04251652E8750C).
516     |2026-08-13 20:30:48 |Normal      |0x0100000F  |Asserted    |DIMM170 installed (SN:80CE04251652E87FCC).
515     |2026-08-13 20:30:48 |Normal      |0x0100000F  |Asserted    |DIMM180 installed (SN:80CE04252942C0CE84).
514     |2026-08-13 20:30:47 |Normal      |0x0100000F  |Asserted    |DIMM0A0 installed (SN:80CE04252942C0D008).
513     |2026-08-13 20:30:47 |Normal      |0x0100000F  |Asserted    |DIMM020 installed (SN:80CE04252942C0E0DD).
512     |2026-08-13 20:30:47 |Normal      |0x0100000F  |Asserted    |DIMM190 installed (SN:80CE04252942C0D077).
511     |2026-08-13 20:30:47 |Normal      |0x0100000F  |Asserted    |DIMM060 installed (SN:80CE04251652E874EA).
510     |2026-08-13 20:30:47 |Normal      |0x0100000F  |Asserted    |DIMM1A0 installed (SN:80CE04252942C0D0D2).
509     |2026-08-13 20:30:47 |Normal      |0x0100000F  |Asserted    |DIMM140 installed (SN:80CE04251652E8750F).
508     |2026-08-13 20:30:46 |Normal      |0x0100000F  |Asserted    |DIMM080 installed (SN:80CE04252942C0D009).
507     |2026-08-13 20:30:46 |Normal      |0x01000041  |Asserted    |CPU Board1 DIMM000 is replaced from SN(80CE0125420229DFD7) to SN(80CE04252942C0CF64) (SN:80CE04252942C0CF64).
506     |2026-08-13 20:30:46 |Normal      |0x0100000F  |Asserted    |DIMM160 installed (SN:80CE04252942C0CF63).
505     |2026-08-13 20:30:46 |Normal      |0x0100000F  |Asserted    |DIMM110 installed (SN:80CE04252942C0D08D).
504     |2026-08-13 20:30:46 |Normal      |0x0100000F  |Asserted    |DIMM050 installed (SN:80CE04252942C0E066).
503     |2026-08-13 20:30:45 |Normal      |0x0100000F  |Asserted    |DIMM090 installed (SN:80CE04252942C0CEF8).
502     |2026-08-13 20:30:45 |Normal      |0x0100000F  |Asserted    |DIMM070 installed (SN:80CE04252942C0DF70).
501     |2026-08-13 20:30:45 |Normal      |0x0100000F  |Asserted    |DIMM150 installed (SN:80CE04252942C0E150).
500     |2026-08-13 20:30:45 |Normal      |0x0100000F  |Asserted    |DIMM120 installed (SN:80CE04252942C0CF26).
499     |2026-08-13 20:30:44 |Normal      |0x0100000F  |Asserted    |DIMM100 installed (SN:80CE04251652E87FCB).
498     |2026-08-13 20:30:44 |Normal      |0x0100000F  |Asserted    |DIMM130 installed (SN:80CE04251652E87BFB).
497     |2026-08-13 20:30:44 |Normal      |0x0100000F  |Asserted    |DIMM0B0 installed (SN:80CE04252942C0E121).
496     |2026-08-13 20:30:43 |Normal      |0x0100000F  |Asserted    |DIMM040 installed (SN:80CE04252942C0CF29).
495     |2026-08-13 20:30:42 |Normal      |0x0100000F  |Asserted    |DIMM030 installed.
494     |2026-08-13 20:30:42 |Normal      |0x0100000F  |Asserted    |DIMM010 installed (SN:80CE04252942C0E067).
493     |2026-08-13 20:25:05 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
492     |2026-08-13 20:25:05 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
491     |2026-08-13 20:02:07 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
490     |2026-08-13 20:02:03 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
489     |2026-08-13 18:06:01 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
488     |2026-08-13 18:04:55 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
487     |2026-08-13 18:04:54 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
486     |2026-08-13 18:04:46 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
485     |2026-08-13 18:04:42 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
484     |2026-08-13 18:01:51 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
483     |2026-08-13 18:00:46 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
482     |2026-08-13 18:00:44 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
481     |2026-08-13 18:00:36 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
480     |2026-08-13 18:00:32 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
479     |2026-08-13 17:57:50 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
478     |2026-08-13 17:56:45 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
477     |2026-08-13 17:56:43 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
476     |2026-08-13 17:56:35 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
475     |2026-08-13 17:56:31 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
474     |2026-08-13 17:53:50 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
473     |2026-08-13 17:52:44 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
472     |2026-08-13 17:52:43 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
471     |2026-08-13 17:50:33 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
470     |2026-08-13 17:50:24 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
469     |2026-08-13 17:36:48 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
468     |2026-08-13 17:35:42 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
467     |2026-08-13 17:35:40 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
466     |2026-08-13 17:35:32 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
465     |2026-08-13 17:35:27 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
464     |2026-08-13 17:32:43 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
463     |2026-08-13 17:31:38 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
462     |2026-08-13 17:31:37 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
461     |2026-08-13 17:30:09 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
460     |2026-08-13 17:29:54 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
459     |2026-08-13 17:29:53 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
458     |2026-08-13 17:29:50 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
457     |2026-08-13 17:29:45 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
456     |2026-08-13 17:29:23 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
455     |2026-08-13 17:28:17 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
454     |2026-08-13 17:28:15 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
453     |2026-08-13 17:28:05 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
452     |2026-08-13 17:28:01 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
451     |2026-08-13 17:25:07 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
450     |2026-08-13 17:24:02 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
449     |2026-08-13 17:24:00 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
448     |2026-08-13 17:23:50 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
447     |2026-08-13 17:23:47 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
446     |2026-08-13 17:21:06 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
445     |2026-08-13 17:20:01 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
444     |2026-08-13 17:20:00 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
443     |2026-08-13 17:11:43 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
442     |2026-08-13 17:11:40 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
441     |2026-08-13 16:22:02 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
440     |2026-08-13 16:20:56 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
439     |2026-08-13 16:20:55 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
438     |2026-08-13 16:16:36 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
437     |2026-08-13 16:16:31 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
436     |2026-08-13 16:14:10 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
435     |2026-08-13 16:13:05 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
434     |2026-08-13 16:13:04 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
433     |2026-08-13 16:12:55 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
432     |2026-08-13 16:12:51 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
431     |2026-08-13 16:09:56 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
430     |2026-08-13 16:08:49 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
429     |2026-08-13 16:08:48 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
428     |2026-08-13 16:08:38 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
427     |2026-08-13 16:08:35 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
426     |2026-08-13 16:05:53 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
425     |2026-08-13 16:04:46 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
424     |2026-08-13 16:04:45 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
423     |2026-08-13 16:02:37 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
422     |2026-08-13 16:02:34 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
421     |2026-08-13 16:01:55 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
420     |2026-08-13 16:00:50 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
419     |2026-08-13 16:00:49 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
418     |2026-08-13 16:00:40 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
417     |2026-08-13 16:00:37 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
416     |2026-08-13 16:00:33 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
415     |2026-08-13 16:00:33 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
414     |2026-08-13 16:00:33 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
413     |2026-08-13 16:00:33 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
412     |2026-08-13 15:59:56 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
411     |2026-08-13 15:59:55 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
410     |2026-08-13 15:59:21 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
409     |2026-08-13 15:59:13 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
408     |2026-08-13 15:57:52 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
407     |2026-08-13 15:56:44 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
406     |2026-08-13 15:56:43 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
405     |2026-08-13 15:56:34 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
404     |2026-08-13 15:56:31 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
403     |2026-08-13 15:56:28 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
402     |2026-08-13 15:56:28 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
401     |2026-08-13 15:56:27 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
400     |2026-08-13 15:56:27 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
399     |2026-08-13 15:55:42 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
398     |2026-08-13 15:55:42 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
397     |2026-08-13 15:55:12 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
396     |2026-08-13 15:55:04 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
395     |2026-08-13 15:53:39 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
394     |2026-08-13 15:52:33 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
393     |2026-08-13 15:52:32 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
392     |2026-08-13 15:52:21 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
391     |2026-08-13 15:52:17 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
390     |2026-08-13 15:52:14 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
389     |2026-08-13 15:52:13 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
388     |2026-08-13 15:51:48 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
387     |2026-08-13 15:51:40 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
386     |2026-08-13 15:49:33 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
385     |2026-08-13 15:48:27 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
384     |2026-08-13 15:48:26 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
383     |2026-08-13 15:47:20 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
382     |2026-08-13 15:47:19 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
381     |2026-08-13 15:47:12 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
380     |2026-08-13 15:47:12 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
379     |2026-08-13 15:47:09 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
378     |2026-08-13 15:47:09 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
377     |2026-08-13 15:47:07 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
376     |2026-08-13 15:47:04 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
375     |2026-08-13 15:46:58 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
374     |2026-08-13 15:46:00 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
373     |2026-08-13 15:46:00 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
372     |2026-08-13 15:46:00 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
371     |2026-08-13 15:46:00 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
370     |2026-08-13 15:46:00 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
369     |2026-08-13 15:46:00 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
368     |2026-08-13 15:45:59 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
367     |2026-08-13 15:45:59 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
366     |2026-08-13 15:45:43 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
365     |2026-08-13 15:44:59 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
364     |2026-08-13 15:44:47 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
363     |2026-08-13 15:44:28 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
362     |2026-08-13 15:40:28 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
361     |2026-08-13 15:40:27 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
360     |2026-08-13 15:40:17 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
359     |2026-08-13 15:40:14 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
358     |2026-08-13 15:37:34 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
357     |2026-08-13 15:36:28 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
356     |2026-08-13 15:36:26 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
355     |2026-08-13 15:33:13 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
354     |2026-08-13 15:33:10 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
353     |2026-08-13 15:30:28 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
352     |2026-08-13 15:29:22 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
351     |2026-08-13 15:29:21 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
350     |2026-08-13 15:28:26 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
349     |2026-08-13 15:25:16 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
348     |2026-08-13 15:24:11 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
347     |2026-08-13 15:24:11 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
346     |2026-08-13 15:24:01 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
345     |2026-08-13 15:23:57 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
344     |2026-08-13 15:23:05 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
343     |2026-08-13 15:21:58 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
342     |2026-08-13 15:21:57 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
341     |2026-08-13 15:21:43 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
340     |2026-08-13 15:20:54 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
339     |2026-08-13 15:20:45 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
338     |2026-08-13 15:20:41 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
337     |2026-08-13 15:20:38 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
336     |2026-08-13 15:20:38 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
335     |2026-08-13 15:20:38 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
334     |2026-08-13 15:20:38 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
333     |2026-08-13 15:20:03 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
332     |2026-08-13 15:20:02 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
331     |2026-08-13 15:19:30 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
330     |2026-08-13 15:19:20 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
329     |2026-08-13 15:17:56 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
328     |2026-08-13 15:16:49 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
327     |2026-08-13 15:16:48 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
326     |2026-08-13 15:16:38 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
325     |2026-08-13 15:16:35 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
324     |2026-08-13 15:16:32 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
323     |2026-08-13 15:16:32 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
322     |2026-08-13 15:16:32 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
321     |2026-08-13 15:16:32 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
320     |2026-08-13 15:15:12 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
319     |2026-08-13 15:15:02 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
318     |2026-08-13 15:14:55 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
317     |2026-08-13 15:14:54 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
316     |2026-08-13 15:13:39 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
315     |2026-08-13 15:12:33 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
314     |2026-08-13 15:12:32 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
313     |2026-08-13 15:12:23 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
312     |2026-08-13 15:12:19 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
311     |2026-08-13 15:12:16 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
310     |2026-08-13 15:12:16 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
309     |2026-08-13 15:12:16 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
308     |2026-08-13 15:12:15 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
307     |2026-08-13 15:11:40 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
306     |2026-08-13 15:11:40 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
305     |2026-08-13 15:11:08 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
304     |2026-08-13 15:11:00 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
303     |2026-08-13 15:09:57 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
302     |2026-08-13 15:09:57 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
301     |2026-08-13 15:09:57 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
300     |2026-08-13 15:09:57 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
299     |2026-08-13 15:09:57 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
298     |2026-08-13 15:09:57 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
297     |2026-08-13 15:09:56 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
296     |2026-08-13 15:09:56 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
295     |2026-08-13 15:09:43 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
294     |2026-08-13 15:08:55 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
293     |2026-08-13 15:08:44 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
292     |2026-08-13 15:08:43 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
291     |2026-08-13 15:04:52 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
290     |2026-08-13 15:04:48 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
289     |2026-08-13 15:04:45 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
288     |2026-08-13 15:04:45 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
287     |2026-08-13 15:04:45 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
286     |2026-08-13 15:04:45 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
285     |2026-08-13 15:04:35 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
284     |2026-08-13 15:04:35 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
283     |2026-08-13 15:04:03 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
282     |2026-08-13 15:03:55 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
281     |2026-08-13 15:02:34 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
280     |2026-08-13 15:01:26 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
279     |2026-08-13 15:01:26 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
278     |2026-08-13 15:01:16 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
277     |2026-08-13 15:01:12 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
276     |2026-08-13 15:01:09 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
275     |2026-08-13 15:01:09 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
274     |2026-08-13 15:01:09 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
273     |2026-08-13 15:01:08 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
272     |2026-08-13 15:00:31 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
271     |2026-08-13 15:00:31 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
270     |2026-08-13 14:59:55 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
269     |2026-08-13 14:59:47 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
268     |2026-08-13 14:58:23 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
267     |2026-08-13 14:57:16 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
266     |2026-08-13 14:57:16 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
265     |2026-08-13 14:57:06 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
264     |2026-08-13 14:57:01 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
263     |2026-08-13 14:56:59 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
262     |2026-08-13 14:56:59 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
261     |2026-08-13 14:56:59 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
260     |2026-08-13 14:56:58 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
259     |2026-08-13 14:56:13 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
258     |2026-08-13 14:56:13 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
257     |2026-08-13 14:55:39 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
256     |2026-08-13 14:55:31 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
255     |2026-08-13 14:54:08 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
254     |2026-08-13 14:53:02 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
253     |2026-08-13 14:53:02 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
252     |2026-08-13 14:52:52 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
251     |2026-08-13 14:52:47 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
250     |2026-08-13 14:52:45 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
249     |2026-08-13 14:52:45 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
248     |2026-08-13 14:52:44 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
247     |2026-08-13 14:52:44 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
246     |2026-08-13 14:52:05 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
245     |2026-08-13 14:52:05 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
244     |2026-08-13 14:51:33 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
243     |2026-08-13 14:51:25 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
242     |2026-08-13 14:50:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
241     |2026-08-13 14:50:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
240     |2026-08-13 14:50:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
239     |2026-08-13 14:50:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
238     |2026-08-13 14:50:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
237     |2026-08-13 14:50:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
236     |2026-08-13 14:50:22 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
235     |2026-08-13 14:50:21 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
234     |2026-08-13 14:50:11 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
233     |2026-08-13 14:49:22 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
232     |2026-08-13 14:49:09 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
231     |2026-08-13 14:49:08 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
230     |2026-08-13 14:45:22 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
229     |2026-08-13 14:45:14 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
228     |2026-08-13 14:33:30 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
227     |2026-08-13 14:33:30 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
226     |2026-08-13 14:33:30 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
225     |2026-08-13 14:33:30 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
224     |2026-08-13 14:33:29 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
223     |2026-08-13 14:33:29 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
222     |2026-08-13 14:33:29 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
221     |2026-08-13 14:33:29 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
220     |2026-08-13 14:32:29 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
219     |2026-08-13 14:32:21 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
218     |2026-08-13 14:32:21 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
217     |2026-08-13 14:32:20 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
216     |2026-08-13 14:32:20 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
215     |2026-08-13 14:32:19 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
214     |2026-08-13 14:32:18 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
213     |2026-08-13 14:32:18 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
212     |2026-08-13 14:32:17 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
211     |2026-08-13 14:32:16 |Major       |0x2C000008  |Deasserted  |The BC85ETHA power STBY_2V5_POWER failure results abnormal power-off.
210     |2026-08-13 14:30:58 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
209     |2026-08-13 14:28:47 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
208     |2026-08-13 14:28:47 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
207     |2026-08-13 14:28:47 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
206     |2026-08-13 14:28:47 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
205     |2026-08-13 14:28:47 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
204     |2026-08-13 14:28:47 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
203     |2026-08-13 14:28:46 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
202     |2026-08-13 14:28:46 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
201     |2026-08-13 14:27:36 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
200     |2026-08-13 14:27:36 |Major       |0x2C000007  |Asserted    |The BC85ETHA power STBY_2V5_POWER failure results abnormal power-off.
199     |2026-08-13 14:27:35 |Minor       |0x1A000056  |Deasserted  |Failed to access the Self-description Record of FanBoard1 CAGE2 (SN:1025CB674875).
198     |2026-08-13 14:26:14 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
197     |2026-08-13 14:21:49 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
196     |2026-08-13 14:21:17 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
195     |2026-08-13 14:21:17 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
194     |2026-08-13 14:21:17 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
193     |2026-08-13 14:21:17 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
192     |2026-08-13 14:21:16 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
191     |2026-08-13 14:21:16 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
190     |2026-08-13 14:21:15 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
189     |2026-08-13 14:21:14 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
188     |2026-08-13 14:21:12 |Minor       |0x1A000056  |Deasserted  |Failed to access the Self-description Record of FanBoard1 OCP Riser11 (SN:1025CB674875).
187     |2026-08-13 14:21:12 |Minor       |0x1A000055  |Asserted    |Failed to access the Self-description Record of FanBoard1 CAGE2 (SN:1025CB674875).
186     |2026-08-13 14:19:58 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
185     |2026-08-13 14:11:05 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
184     |2026-08-13 14:11:05 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
183     |2026-08-13 14:11:05 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
182     |2026-08-13 14:11:05 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
181     |2026-08-13 14:11:04 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
180     |2026-08-13 14:11:04 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
179     |2026-08-13 14:11:04 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
178     |2026-08-13 14:11:04 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
177     |2026-08-13 14:10:25 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
176     |2026-08-13 14:09:50 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
175     |2026-08-13 14:09:49 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
174     |2026-08-13 14:09:49 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
173     |2026-08-13 14:09:49 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
172     |2026-08-13 14:09:49 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
171     |2026-08-13 14:09:48 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
170     |2026-08-13 14:09:48 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
169     |2026-08-13 14:09:48 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
168     |2026-08-13 14:09:46 |Minor       |0x1A000055  |Asserted    |Failed to access the Self-description Record of FanBoard1 OCP Riser11 (SN:1025CB674875).
167     |2026-08-13 14:08:33 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
166     |2026-08-11 16:14:23 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
165     |2026-08-11 16:13:17 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
164     |2026-08-11 16:13:16 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
163     |2026-08-11 16:13:08 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
162     |2026-08-11 16:13:03 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
161     |2026-08-11 16:10:09 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
160     |2026-08-11 16:09:01 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
159     |2026-08-11 16:09:01 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
158     |2026-08-11 16:08:51 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
157     |2026-08-11 16:08:47 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
156     |2026-08-11 16:06:03 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
155     |2026-08-11 16:04:56 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
154     |2026-08-11 16:04:55 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
153     |2026-08-11 16:04:46 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
152     |2026-08-11 16:04:43 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
151     |2026-08-11 16:02:11 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
150     |2026-08-11 16:01:00 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
149     |2026-08-11 16:01:00 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
148     |2026-08-11 16:00:47 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
147     |2026-08-11 16:00:44 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
146     |2026-08-11 15:35:56 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
145     |2026-08-11 15:34:50 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
144     |2026-08-11 15:34:49 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
143     |2026-08-11 15:34:41 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
142     |2026-08-11 15:34:36 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
141     |2026-08-11 15:31:53 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
140     |2026-08-11 15:30:47 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
139     |2026-08-11 15:30:46 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
138     |2026-08-11 15:30:38 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
137     |2026-08-11 15:30:34 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
136     |2026-08-11 15:27:52 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
135     |2026-08-11 15:26:40 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
134     |2026-08-11 15:26:39 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
133     |2026-08-11 15:26:31 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
132     |2026-08-11 15:26:26 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
131     |2026-08-11 15:23:37 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
130     |2026-08-11 15:22:29 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
129     |2026-08-11 15:22:28 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
128     |2026-08-11 15:22:24 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
127     |2026-08-11 15:22:20 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
126     |2026-08-11 15:16:31 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
125     |2026-08-11 15:15:24 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
124     |2026-08-11 15:15:23 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
123     |2026-08-11 15:15:15 |Major       |0x28000048  |Deasserted  |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
122     |2026-08-11 15:15:10 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
121     |2026-08-11 15:15:07 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
120     |2026-08-11 15:15:07 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
119     |2026-08-11 15:15:07 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
118     |2026-08-11 15:15:07 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
117     |2026-08-11 15:13:47 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
116     |2026-08-11 15:13:39 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
115     |2026-08-11 15:13:32 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
114     |2026-08-11 15:13:31 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
113     |2026-08-11 15:12:13 |Major       |0x28000047  |Asserted    |HCCS link of CPU0 PCB macro7 on CPU board 1 failed.
112     |2026-08-11 15:11:08 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
111     |2026-08-11 15:11:07 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
110     |2026-08-11 15:10:58 |Major       |0x28000048  |Deasserted  |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
109     |2026-08-11 15:10:54 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
108     |2026-08-11 15:10:51 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
107     |2026-08-11 15:10:51 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
106     |2026-08-11 15:10:51 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
105     |2026-08-11 15:10:51 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
104     |2026-08-11 15:09:47 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
103     |2026-08-11 15:09:41 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
102     |2026-08-11 15:09:32 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
101     |2026-08-11 15:09:31 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
100     |2026-08-11 15:08:08 |Major       |0x28000047  |Asserted    |HCCS link of CPU1 PCB macro0 on CPU board 1 failed.
99      |2026-08-11 15:07:01 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
98      |2026-08-11 15:07:00 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
97      |2026-08-11 15:06:47 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
96      |2026-08-11 15:06:44 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU1) temperature.
95      |2026-08-11 15:06:44 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
94      |2026-08-11 15:06:44 |Minor       |0x01000040  |Deasserted  |Failed to obtain data of the memory (CPU0) temperature.
93      |2026-08-11 15:06:44 |Minor       |0x00000024  |Deasserted  |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
92      |2026-08-11 15:05:56 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 1(CpuBoard1 CPU1) core temperature.
91      |2026-08-11 15:05:50 |Minor       |0x00000023  |Asserted    |Failed to obtain data of the CPU 0(CpuBoard1 CPU0) core temperature.
90      |2026-08-11 15:05:43 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU1) temperature.
89      |2026-08-11 15:05:42 |Minor       |0x0100003F  |Asserted    |Failed to obtain data of the memory (CPU0) temperature.
88      |2026-08-11 15:02:54 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
87      |2026-08-11 15:02:45 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
86      |2026-08-11 15:02:41 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
85      |2026-08-11 14:54:35 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
84      |2026-08-11 14:54:35 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
83      |2026-08-11 14:54:35 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
82      |2026-08-11 14:54:35 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
81      |2026-08-11 14:54:34 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
80      |2026-08-11 14:54:34 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
79      |2026-08-11 14:54:34 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
78      |2026-08-11 14:54:34 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
77      |2026-08-11 14:51:59 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
76      |2026-08-11 14:51:35 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
75      |2026-08-11 14:51:35 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
74      |2026-08-11 14:51:33 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
73      |2026-08-11 14:51:33 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
72      |2026-08-11 14:51:33 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
71      |2026-08-11 14:51:32 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
70      |2026-08-11 14:51:32 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
69      |2026-08-11 14:51:32 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
68      |2026-08-11 14:50:11 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
67      |2026-08-11 14:46:58 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
66      |2026-08-11 14:46:58 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
65      |2026-08-11 14:46:58 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
64      |2026-08-11 14:46:58 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
63      |2026-08-11 14:46:58 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
62      |2026-08-11 14:46:58 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
61      |2026-08-11 14:46:57 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
60      |2026-08-11 14:46:57 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
59      |2026-08-11 14:44:07 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
58      |2026-08-11 14:43:58 |Major       |0x05000004  |Deasserted  |The CPLD 1 self-check result of the Disk backplane BC85NHBA is abnormal.
57      |2026-08-11 14:43:52 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
56      |2026-08-11 14:43:51 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
55      |2026-08-11 14:43:51 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
54      |2026-08-11 14:43:50 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
53      |2026-08-11 14:43:50 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
52      |2026-08-11 14:43:50 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
51      |2026-08-11 14:43:48 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
50      |2026-08-11 14:43:48 |Major       |0x28000036  |Deasserted  |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
49      |2026-08-11 14:42:22 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
48      |2026-08-11 14:40:00 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
47      |2026-08-11 08:55:16 |Critical    |0x0300000E  |Deasserted  |The AC/DC input of PSU 1 is lost or out-of-range (SN:2102312YKRJVRA038523, BN:02312YKR).
46      |2026-08-11 08:45:50 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
45      |2026-08-11 08:45:46 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
44      |2026-08-11 08:45:38 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
43      |2026-08-10 17:09:15 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
42      |2026-08-10 17:09:11 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
41      |2026-08-10 17:09:02 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
40      |2026-08-10 17:07:57 |Major       |0x05000003  |Asserted    |The CPLD 1 self-check result of the Disk backplane BC85NHBA is abnormal.
39      |2026-08-10 16:57:20 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-08-10 16:54:20 UTC, The power has been already restored.
38      |2026-08-10 16:57:03 |Critical    |0x0300000D  |Asserted    |The AC/DC input of PSU 1 is lost or out-of-range (SN:2102312YKRJVRA038523, BN:02312YKR).
37      |2026-08-10 16:56:24 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
36      |2026-08-10 16:56:24 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
35      |2026-08-10 16:56:24 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
34      |2026-08-10 16:56:24 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
33      |2026-08-10 16:56:24 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
32      |2026-08-10 16:56:24 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
31      |2026-08-10 16:56:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
30      |2026-08-10 16:56:23 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
29      |2026-08-10 16:55:09 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
28      |2026-08-10 16:54:49 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
27      |2026-08-10 16:54:48 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
26      |2026-08-10 16:54:34 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
25      |2026-08-10 16:46:52 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-08-10 16:43:52 UTC, The power has been already restored.
24      |2026-08-10 16:45:59 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC8 of BCU1 is not supported.
23      |2026-08-10 16:45:59 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC9 of BCU1 is not supported.
22      |2026-08-10 16:45:59 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC11 of BCU1 is not supported.
21      |2026-08-10 16:45:59 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC9 of BCU1 is not supported.
20      |2026-08-10 16:45:59 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC10 of BCU1 is not supported.
19      |2026-08-10 16:45:58 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC7 of BCU1 is not supported.
18      |2026-08-10 16:45:58 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU1 UBC6 of BCU1 is not supported.
17      |2026-08-10 16:45:58 |Major       |0x28000035  |Asserted    |The unit 00000001030302084145 linked to connector CPU0 UBC8 of BCU1 is not supported.
16      |2026-08-10 16:45:06 |Normal      |0x2400000B  |Asserted    |CPU Board 1 is replaced from SN(102615362795) to SN(102678749486) (SN:102678749486).
15      |2026-08-10 16:45:05 |Normal      |0x03000043  |Asserted    |PSU 1 is replaced from SN(2102312HGYW0N6002827) to SN(2102312YKRJVRA038523) (SN:2102312YKRJVRA038523, BN:02312YKR).
14      |2026-08-10 16:45:01 |Critical    |0x0300000D  |Asserted    |The AC/DC input of PSU 1 is lost or out-of-range (SN:2102312YKRJVRA038523, BN:02312YKR).
13      |2026-08-10 16:44:57 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
12      |2026-08-10 16:44:24 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
11      |2026-08-10 16:44:24 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
10      |2026-08-10 16:44:08 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
9       |2026-01-14 15:04:56 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
8       |2026-01-14 15:04:55 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
7       |2026-01-14 15:03:39 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
6       |2026-01-14 15:03:11 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
5       |2026-01-14 15:03:11 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
4       |2026-01-14 15:03:10 |Normal      |0x31000003  |Asserted    |The UID button on the panel is pressed.
3       |2026-01-14 15:02:57 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
2       |2026-01-14 13:59:45 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
1       |2026-01-14 13:59:15 |Normal      |0x1A00000F  |Asserted    |iBMC event records are cleared.
