ID      |Generation Time     |Severity    |Event Code  |Status      |Event Description
538     |2026-06-15 11:39:24 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-15 11:33:43 UTC, The power has been already restored.
537     |2026-06-15 11:37:19 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
536     |2026-06-15 11:37:18 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
535     |2026-06-15 11:36:56 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
534     |2026-06-15 11:36:06 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
533     |2026-06-15 11:33:43 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
532     |2026-06-15 11:16:48 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-15 11:13:48 UTC, The power has been already restored.
531     |2026-06-15 11:14:46 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
530     |2026-06-15 11:14:45 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
529     |2026-06-15 11:14:22 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
528     |2026-06-15 11:13:08 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
527     |2026-06-15 11:10:35 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 2 disconnected.
526     |2026-06-15 11:10:24 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
525     |2026-06-15 10:59:31 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-15 10:56:31 UTC, The power has been already restored.
524     |2026-06-15 10:57:59 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
523     |2026-06-15 10:57:58 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
522     |2026-06-15 10:56:50 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
521     |2026-06-15 10:56:24 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
520     |2026-06-15 10:47:27 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 2 disconnected.
519     |2026-06-15 10:47:15 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
518     |2026-06-15 09:18:45 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF221Q) Port 2 disconnected.
517     |2026-06-15 09:18:27 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 2 disconnected.
516     |2026-06-15 09:18:12 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
515     |2026-06-15 08:12:31 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF221Q) Port 2 disconnected.
514     |2026-06-15 08:12:07 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 2 disconnected.
513     |2026-06-15 08:11:57 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
512     |2026-06-15 07:36:22 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF221Q) Port 2 disconnected.
511     |2026-06-15 07:35:51 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
510     |2026-06-15 07:34:27 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 2 disconnected.
509     |2026-06-15 06:56:48 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF221Q) Port 2 disconnected.
508     |2026-06-15 06:56:16 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
507     |2026-06-15 06:54:53 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 2 disconnected.
506     |2026-06-15 02:50:50 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF221Q) Port 2 disconnected.
505     |2026-06-15 02:50:01 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
504     |2026-06-15 02:50:00 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
503     |2026-06-12 08:56:41 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
502     |2026-06-12 08:55:18 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 2 disconnected.
501     |2026-06-12 08:29:32 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-12 08:26:32 UTC, The power has been already restored.
500     |2026-06-12 08:28:01 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
499     |2026-06-12 08:28:01 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
498     |2026-06-12 08:27:39 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
497     |2026-06-12 08:26:48 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
496     |2026-06-12 08:24:34 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
495     |2026-06-12 08:23:32 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 2 disconnected.
494     |2026-06-12 08:06:26 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-12 07:50:27 UTC, The power has been already restored.
493     |2026-06-12 08:05:00 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
492     |2026-06-12 08:04:34 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
491     |2026-06-12 08:04:34 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
490     |2026-06-12 08:04:26 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
489     |2026-06-12 08:03:21 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
488     |2026-06-12 07:49:57 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
487     |2026-06-12 07:48:36 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 2 disconnected.
486     |2026-06-12 07:43:17 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-12 07:25:32 UTC, The power has been already restored.
485     |2026-06-12 07:41:59 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
484     |2026-06-12 07:40:40 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
483     |2026-06-12 07:40:39 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
482     |2026-06-12 07:23:22 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 2 disconnected.
481     |2026-06-12 07:23:10 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
480     |2026-06-12 07:05:25 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 3 disconnected.
479     |2026-06-12 07:04:19 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF221Q) Port 3 disconnected.
478     |2026-06-12 07:04:19 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 4 disconnected.
477     |2026-06-12 06:58:14 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF221Q) Port 4 disconnected.
476     |2026-06-12 06:57:55 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 3 disconnected.
475     |2026-06-12 06:35:12 |Minor       |0x0F00001E  |Deasserted  |The MCU communication error occurs on PCIe riser card2 (BN:0302044499).
474     |2026-06-12 06:35:07 |Minor       |0x0F00001D  |Asserted    |The MCU communication error occurs on PCIe riser card2 (BN:0302044499).
473     |2026-06-12 06:34:48 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
472     |2026-06-12 06:30:56 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF221Q) Port 3 disconnected.
471     |2026-06-12 06:30:56 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 4 disconnected.
470     |2026-06-12 06:30:38 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 3 disconnected.
469     |2026-06-12 06:30:38 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF221Q) Port 4 disconnected.
468     |2026-06-12 06:21:36 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 4 disconnected.
467     |2026-06-12 02:57:40 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-12 02:54:39 UTC, The power has been already restored.
466     |2026-06-12 02:56:05 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
465     |2026-06-12 02:55:42 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
464     |2026-06-12 02:54:58 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
463     |2026-06-12 02:45:42 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
462     |2026-06-11 11:25:27 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-11 11:22:27 UTC, The power has been already restored.
461     |2026-06-11 11:23:55 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
460     |2026-06-11 11:23:33 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
459     |2026-06-11 11:23:32 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
458     |2026-06-11 11:22:46 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
457     |2026-06-11 11:16:36 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
456     |2026-06-11 08:40:23 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-11 08:35:28 UTC, The power has been already restored.
455     |2026-06-11 08:38:53 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
454     |2026-06-11 08:38:53 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
453     |2026-06-11 08:38:30 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
452     |2026-06-11 08:37:25 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
451     |2026-06-11 08:34:29 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
450     |2026-06-11 08:28:23 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
449     |2026-06-11 06:50:33 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-11 06:24:10 UTC, The power has been already restored.
448     |2026-06-11 06:49:06 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
447     |2026-06-11 06:49:06 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
446     |2026-06-11 06:48:21 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
445     |2026-06-11 06:47:30 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
444     |2026-06-11 06:47:29 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
443     |2026-06-11 06:24:11 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
442     |2026-06-11 06:23:32 |Normal      |0x1A000029  |Asserted    |BMC time is stepped by more than 480 minutes.
441     |2026-06-11 11:03:33 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
440     |2026-06-11 11:03:32 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
439     |2026-06-09 17:14:38 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
438     |2026-06-09 17:13:14 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
437     |2026-06-09 15:27:28 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
436     |2026-06-09 15:27:26 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
435     |2026-06-09 14:15:36 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
434     |2026-06-09 14:15:34 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
433     |2026-06-09 09:03:59 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
432     |2026-06-09 09:03:24 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
431     |2026-06-08 17:32:43 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-08 17:15:30 UTC, The power has been already restored.
430     |2026-06-08 17:31:23 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
429     |2026-06-08 17:30:56 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
428     |2026-06-08 17:30:47 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
427     |2026-06-08 17:30:13 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
426     |2026-06-08 17:29:44 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
425     |2026-06-08 17:15:07 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
424     |2026-06-08 17:13:56 |Normal      |0x29000001  |Asserted    |NIC 1 (SF221Q) Port 4 disconnected.
423     |2026-06-08 17:11:21 |Normal      |0x1A000029  |Asserted    |BMC time is stepped by more than 479 minutes.
422     |2026-06-08 09:03:39 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
421     |2026-06-08 09:03:39 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
420     |2026-06-08 09:03:33 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
419     |2026-06-08 08:59:12 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
418     |2026-06-08 08:57:53 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-08 08:51:43 UTC, The power has been already restored.
417     |2026-06-08 08:56:57 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
416     |2026-06-08 08:56:56 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
415     |2026-06-08 08:56:29 |Normal      |0x0D000015  |Asserted    |The NIC 1 is replaced from SN(102579066733) to SN(W02630658900) (SN:W02630658900).
414     |2026-06-08 08:56:27 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
413     |2026-06-08 08:56:02 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
412     |2026-06-08 08:55:19 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
411     |2026-06-08 08:54:48 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
410     |2026-06-08 08:48:06 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
409     |2026-06-08 08:47:35 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
408     |2026-06-08 08:42:41 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
407     |2026-06-08 08:42:41 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
406     |2026-06-08 08:42:35 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
405     |2026-06-08 08:27:45 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
404     |2026-06-08 08:24:43 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
403     |2026-06-08 08:24:42 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
402     |2026-06-08 08:23:19 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
401     |2026-06-08 05:55:14 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
400     |2026-06-08 05:55:13 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
399     |2026-06-08 05:52:16 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
398     |2026-06-08 05:52:13 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
397     |2026-06-08 05:52:13 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
396     |2026-06-08 05:51:53 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
395     |2026-06-08 05:45:46 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
394     |2026-06-08 05:33:54 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-08 05:30:54 UTC, The power has been already restored.
393     |2026-06-08 05:32:36 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
392     |2026-06-08 05:32:35 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
391     |2026-06-08 05:32:35 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
390     |2026-06-08 05:31:22 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
389     |2026-06-08 05:30:52 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
388     |2026-06-08 03:17:31 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
387     |2026-06-08 03:17:27 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
386     |2026-06-08 03:17:25 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
385     |2026-06-08 03:17:24 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
384     |2026-06-08 03:17:17 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
383     |2026-06-08 03:16:54 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
382     |2026-06-08 03:14:35 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
381     |2026-06-08 02:09:54 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-08 01:58:43 UTC, The power has been already restored.
380     |2026-06-08 02:08:34 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
379     |2026-06-08 02:06:54 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
378     |2026-06-08 02:06:52 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
377     |2026-06-08 01:57:15 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
376     |2026-06-08 01:45:00 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
375     |2026-06-08 01:45:00 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
374     |2026-06-08 01:43:59 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
373     |2026-06-08 01:43:57 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x10.
372     |2026-06-08 01:40:59 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
371     |2026-06-08 01:40:59 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
370     |2026-06-08 01:40:14 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
369     |2026-06-08 01:40:07 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
368     |2026-06-08 01:22:56 |Major       |0x29000014  |Deasserted  |Abnormal Rx signal of optical module is detected on Port 2 on NIC 1 (SF223D-H).
367     |2026-06-08 01:20:50 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
366     |2026-06-08 01:19:48 |Major       |0x29000014  |Deasserted  |Abnormal Rx signal of optical module is detected on Port 1 on NIC 1 (SF223D-H).
365     |2026-06-08 01:19:25 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
364     |2026-06-04 02:59:21 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-04 02:48:50 UTC, The power has been already restored.
363     |2026-06-04 02:59:09 |Major       |0x29000013  |Asserted    |Abnormal Rx signal of optical module is detected on Port 2 on NIC 1 (SF223D-H).
362     |2026-06-04 02:59:08 |Major       |0x29000013  |Asserted    |Abnormal Rx signal of optical module is detected on Port 1 on NIC 1 (SF223D-H).
361     |2026-06-04 02:57:54 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
360     |2026-06-04 02:57:30 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
359     |2026-06-04 02:56:47 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
358     |2026-06-04 02:48:50 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
357     |2026-06-03 08:12:08 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
356     |2026-06-03 08:08:24 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
355     |2026-06-03 06:18:47 |Major       |0x29000013  |Asserted    |Abnormal Rx signal of optical module is detected on Port 2 on NIC 1 (SF223D-H).
354     |2026-06-03 06:18:44 |Major       |0x29000013  |Asserted    |Abnormal Rx signal of optical module is detected on Port 1 on NIC 1 (SF223D-H).
353     |2026-06-03 06:17:14 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
352     |2026-06-03 06:17:13 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
351     |2026-06-03 06:07:22 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
350     |2026-06-03 01:50:52 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
349     |2026-06-03 01:50:49 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
348     |2026-06-03 01:46:13 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-06-03 01:09:02 UTC, The power has been already restored.
347     |2026-06-03 01:45:30 |Major       |0x29000013  |Asserted    |Abnormal Rx signal of optical module is detected on Port 2 on NIC 1 (SF223D-H).
346     |2026-06-03 01:45:28 |Major       |0x29000013  |Asserted    |Abnormal Rx signal of optical module is detected on Port 1 on NIC 1 (SF223D-H).
345     |2026-06-03 01:44:56 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
344     |2026-06-03 01:44:55 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
343     |2026-06-03 01:44:15 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
342     |2026-06-03 01:43:08 |Normal      |0x1A00000D  |Asserted    |BMC is restarted after AC power supply is restored.
341     |2026-06-02 09:09:24 |Major       |0x29000014  |Deasserted  |Abnormal Rx signal of optical module is detected on Port 1 on NIC 1 (SF223D-H).
340     |2026-06-02 09:07:54 |Major       |0x29000014  |Deasserted  |Abnormal Rx signal of optical module is detected on Port 2 on NIC 1 (SF223D-H).
339     |2026-06-02 09:06:57 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
338     |2026-06-02 06:57:25 |Major       |0x29000013  |Asserted    |Abnormal Rx signal of optical module is detected on Port 2 on NIC 1 (SF223D-H).
337     |2026-06-02 06:57:22 |Major       |0x29000013  |Asserted    |Abnormal Rx signal of optical module is detected on Port 1 on NIC 1 (SF223D-H).
336     |2026-06-02 06:56:29 |Major       |0x29000014  |Deasserted  |Abnormal Rx signal of optical module is detected on Port 2 on NIC 1 (SF223D-H).
335     |2026-06-02 06:56:26 |Major       |0x29000014  |Deasserted  |Abnormal Rx signal of optical module is detected on Port 1 on NIC 1 (SF223D-H).
334     |2026-06-02 06:56:07 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
333     |2026-06-02 06:30:38 |Normal      |0x1A00006F  |Asserted    |The BMC is reset, with the cause code of 0x2.
332     |2026-06-02 06:29:15 |Normal      |0x1A000021  |Asserted    |BMC is reset and started.
331     |2026-06-02 03:08:25 |Major       |0x29000013  |Asserted    |Abnormal Rx signal of optical module is detected on Port 2 on NIC 1 (SF223D-H).
330     |2026-06-02 03:08:24 |Major       |0x29000013  |Asserted    |Abnormal Rx signal of optical module is detected on Port 1 on NIC 1 (SF223D-H).
329     |2026-06-02 03:07:39 |Normal      |0x1A000021  |Asserted    |openUBMC is reset and started.
328     |2026-06-02 03:01:02 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
327     |2026-06-02 02:54:34 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
326     |2026-06-02 02:46:58 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
325     |2026-06-02 02:39:50 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
324     |2026-06-02 02:29:38 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
323     |2026-05-29 07:53:58 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
322     |2026-05-29 07:38:29 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-29 07:35:29 UTC, The power has been already restored.
321     |2026-05-29 07:37:25 |Normal      |0x12000006  |Deasserted  |Chassis cover is open.
320     |2026-05-29 07:37:23 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
319     |2026-05-29 07:37:07 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
318     |2026-05-29 07:36:56 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
317     |2026-05-29 07:36:53 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
316     |2026-05-29 07:21:36 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
315     |2026-05-29 02:09:48 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
314     |2026-05-28 09:13:46 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
313     |2026-05-28 08:15:25 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
312     |2026-05-28 08:11:03 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
311     |2026-05-28 08:11:02 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
310     |2026-05-28 08:10:47 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
309     |2026-05-28 03:48:59 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
308     |2026-05-28 03:20:34 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
307     |2026-05-28 03:20:34 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
306     |2026-05-28 03:20:19 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
305     |2026-05-28 03:18:02 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
304     |2026-05-28 03:14:58 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
303     |2026-05-28 03:14:58 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
302     |2026-05-28 03:14:43 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
301     |2026-05-28 03:01:50 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
300     |2026-05-28 03:01:49 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
299     |2026-05-28 03:01:34 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
298     |2026-05-28 02:46:59 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
297     |2026-05-28 02:46:59 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
296     |2026-05-28 02:46:46 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
295     |2026-05-28 02:26:26 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
294     |2026-05-28 02:26:26 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
293     |2026-05-28 02:26:11 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
292     |2026-05-28 02:24:42 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
291     |2026-05-28 02:00:02 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
290     |2026-05-28 01:58:33 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-28 01:55:33 UTC, The power has been already restored.
289     |2026-05-28 01:57:09 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
288     |2026-05-28 01:56:55 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
287     |2026-05-28 01:56:54 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
286     |2026-05-28 01:54:20 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
285     |2026-05-28 01:48:31 |Minor       |0x0D00001A  |Deasserted  |Failed to obtain data of the NIC optical module temperature.
284     |2026-05-28 01:48:20 |Minor       |0x0D000019  |Asserted    |Failed to obtain data of the NIC optical module temperature.
283     |2026-05-28 01:48:10 |Minor       |0x0D00001A  |Deasserted  |Failed to obtain data of the NIC optical module temperature.
282     |2026-05-28 01:47:50 |Minor       |0x0D000019  |Asserted    |Failed to obtain data of the NIC optical module temperature.
281     |2026-05-28 01:45:37 |Minor       |0x0D00001A  |Deasserted  |Failed to obtain data of the NIC optical module temperature.
280     |2026-05-28 01:45:27 |Minor       |0x0D000019  |Asserted    |Failed to obtain data of the NIC optical module temperature.
279     |2026-05-28 01:30:42 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
278     |2026-05-28 01:10:05 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
277     |2026-05-28 01:05:35 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
276     |2026-05-28 00:59:10 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-28 00:49:17 UTC, The power has been already restored.
275     |2026-05-28 00:58:04 |Normal      |0x12000006  |Deasserted  |Chassis cover is open.
274     |2026-05-28 00:58:02 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
273     |2026-05-28 00:57:38 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
272     |2026-05-28 00:57:35 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
271     |2026-05-28 00:57:30 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
270     |2026-05-28 00:53:09 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
269     |2026-05-28 00:53:08 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
268     |2026-05-28 00:53:07 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
267     |2026-05-28 00:53:00 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
266     |2026-05-28 00:52:53 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
265     |2026-05-28 00:52:52 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
264     |2026-05-28 00:52:51 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
263     |2026-05-28 00:52:50 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
262     |2026-05-28 00:52:49 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
261     |2026-05-28 00:52:48 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
260     |2026-05-28 00:52:48 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
259     |2026-05-28 00:51:54 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
258     |2026-05-28 00:51:53 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
257     |2026-05-28 00:51:52 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
256     |2026-05-28 00:51:50 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
255     |2026-05-28 00:51:50 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
254     |2026-05-28 00:51:49 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
253     |2026-05-28 00:51:43 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
252     |2026-05-28 00:51:42 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
251     |2026-05-28 00:51:41 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
250     |2026-05-28 00:51:40 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
249     |2026-05-28 00:51:39 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
248     |2026-05-28 00:51:38 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
247     |2026-05-28 00:51:37 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
246     |2026-05-28 00:51:26 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
245     |2026-05-28 00:51:26 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
244     |2026-05-28 00:51:25 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
243     |2026-05-28 00:51:24 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
242     |2026-05-28 00:51:22 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
241     |2026-05-28 00:51:22 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
240     |2026-05-28 00:50:54 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
239     |2026-05-28 00:50:53 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
238     |2026-05-28 00:50:52 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
237     |2026-05-28 00:50:52 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
236     |2026-05-28 00:50:52 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
235     |2026-05-28 00:50:51 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
234     |2026-05-28 00:50:49 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
233     |2026-05-28 00:50:44 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
232     |2026-05-28 00:46:24 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
231     |2026-05-28 00:46:24 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
230     |2026-05-28 00:46:22 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
229     |2026-05-28 00:46:21 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
228     |2026-05-28 00:46:18 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
227     |2026-05-28 00:46:16 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
226     |2026-05-28 00:46:11 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
225     |2026-05-28 00:45:59 |Normal      |0x02000023  |Asserted    |The disk Disk1 is replaced from SN(2025082800559) to SN(035MQBP0R8708785) (SN:035MQBP0R8708785).
224     |2026-05-28 00:45:46 |Normal      |0x02000023  |Asserted    |The disk Disk0 is replaced from SN(S45RNC0T611284) to SN(035MQBZER7012170) (SN:035MQBZER7012170).
223     |2026-05-28 00:44:17 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-28 00:41:17 UTC, The power has been already restored.
222     |2026-05-28 00:43:15 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
221     |2026-05-28 00:43:14 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
220     |2026-05-28 00:43:13 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
219     |2026-05-28 00:43:13 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
218     |2026-05-28 00:43:10 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
217     |2026-05-28 00:43:07 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
216     |2026-05-28 00:42:52 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
215     |2026-05-28 00:42:50 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
214     |2026-05-28 00:42:41 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
213     |2026-05-28 00:42:37 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
212     |2026-05-27 13:20:17 |Normal      |0x12000006  |Deasserted  |Chassis cover is open.
211     |2026-05-27 13:19:35 |Normal      |0x02000005  |Asserted    |The disk Disk0 removed (SN:S45RNC0T611284).
210     |2026-05-27 13:19:31 |Normal      |0x02000005  |Asserted    |The disk Disk1 removed (SN:2025082800559).
209     |2026-05-27 13:19:05 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
208     |2026-05-27 13:11:46 |Normal      |0x12000006  |Deasserted  |Chassis cover is open.
207     |2026-05-27 13:06:52 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
206     |2026-05-27 13:06:51 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
205     |2026-05-27 13:06:50 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
204     |2026-05-27 13:06:50 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
203     |2026-05-27 13:06:49 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
202     |2026-05-27 13:06:47 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
201     |2026-05-27 13:06:47 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
200     |2026-05-27 13:05:51 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
199     |2026-05-27 12:28:36 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-27 12:25:36 UTC, The power has been already restored.
198     |2026-05-27 12:27:29 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
197     |2026-05-27 12:27:13 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
196     |2026-05-27 12:27:03 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
195     |2026-05-27 12:27:01 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
194     |2026-05-27 12:13:44 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
193     |2026-05-27 12:09:18 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
192     |2026-05-27 12:05:28 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
191     |2026-05-27 12:01:52 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
190     |2026-05-27 11:59:04 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
189     |2026-05-27 09:30:10 |Normal      |0x12000006  |Deasserted  |Chassis cover is open.
188     |2026-05-27 09:09:09 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-27 09:06:09 UTC, The power has been already restored.
187     |2026-05-27 09:07:59 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
186     |2026-05-27 09:07:47 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
185     |2026-05-27 09:07:33 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
184     |2026-05-27 09:07:32 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
183     |2026-05-27 09:04:08 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
182     |2026-05-27 09:04:04 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
181     |2026-05-27 09:04:04 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
180     |2026-05-27 09:04:03 |Critical    |0x2C000088  |Deasserted  |BIOS secure boot failed.
179     |2026-05-27 09:04:03 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
178     |2026-05-27 09:03:58 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
177     |2026-05-27 09:03:45 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
176     |2026-05-27 09:03:39 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-27 08:55:50 UTC, The power has been already restored.
175     |2026-05-27 09:03:38 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
174     |2026-05-27 09:03:05 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
173     |2026-05-27 09:03:01 |Critical    |0x2C000087  |Asserted    |BIOS secure boot failed.
172     |2026-05-27 09:02:12 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
171     |2026-05-27 09:02:04 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
170     |2026-05-27 09:02:00 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
169     |2026-05-27 08:50:09 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
168     |2026-05-27 06:43:46 |Minor       |0x0D00001A  |Deasserted  |Failed to obtain data of the NIC optical module temperature.
167     |2026-05-27 06:43:35 |Minor       |0x0D000019  |Asserted    |Failed to obtain data of the NIC optical module temperature.
166     |2026-05-27 06:23:37 |Minor       |0x0D00001A  |Deasserted  |Failed to obtain data of the NIC optical module temperature.
165     |2026-05-27 06:23:27 |Minor       |0x0D000019  |Asserted    |Failed to obtain data of the NIC optical module temperature.
164     |2026-05-27 05:55:27 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-27 05:40:58 UTC, The power has been already restored.
163     |2026-05-27 05:54:19 |Normal      |0x12000006  |Deasserted  |Chassis cover is open.
162     |2026-05-27 05:54:16 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
161     |2026-05-27 05:54:05 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
160     |2026-05-27 05:53:52 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
159     |2026-05-27 05:53:51 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
158     |2026-05-27 05:43:54 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
157     |2026-05-27 05:43:53 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
156     |2026-05-27 05:43:47 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
155     |2026-05-27 04:42:34 |Minor       |0x0D00001A  |Deasserted  |Failed to obtain data of the NIC optical module temperature.
154     |2026-05-27 04:42:24 |Minor       |0x0D000019  |Asserted    |Failed to obtain data of the NIC optical module temperature.
153     |2026-05-27 03:49:37 |Minor       |0x0D00001A  |Deasserted  |Failed to obtain data of the NIC optical module temperature.
152     |2026-05-27 03:48:26 |Minor       |0x0D000019  |Asserted    |Failed to obtain data of the NIC optical module temperature.
151     |2026-05-27 03:36:05 |Minor       |0x0D00001A  |Deasserted  |Failed to obtain data of the NIC optical module temperature.
150     |2026-05-27 03:27:07 |Minor       |0x0D000019  |Asserted    |Failed to obtain data of the NIC optical module temperature.
149     |2026-05-27 03:22:51 |Minor       |0x0D00001A  |Deasserted  |Failed to obtain data of the NIC optical module temperature.
148     |2026-05-27 03:21:50 |Minor       |0x0D000019  |Asserted    |Failed to obtain data of the NIC optical module temperature.
147     |2026-05-27 03:20:59 |Minor       |0x0D00001A  |Deasserted  |Failed to obtain data of the NIC optical module temperature.
146     |2026-05-27 03:20:18 |Minor       |0x0D000019  |Asserted    |Failed to obtain data of the NIC optical module temperature.
145     |2026-05-27 02:45:58 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-27 02:42:58 UTC, The power has been already restored.
144     |2026-05-27 02:45:26 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
143     |2026-05-27 02:45:23 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
142     |2026-05-27 02:45:22 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
141     |2026-05-27 02:45:15 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
140     |2026-05-27 02:44:50 |Normal      |0x12000006  |Deasserted  |Chassis cover is open.
139     |2026-05-27 02:44:49 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
138     |2026-05-27 02:44:25 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
137     |2026-05-27 02:44:24 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
136     |2026-05-27 02:44:21 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
135     |2026-05-27 02:44:16 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
134     |2026-05-27 02:37:29 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
133     |2026-05-27 02:36:33 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
132     |2026-05-27 02:36:32 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
131     |2026-05-27 02:36:26 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
130     |2026-05-27 02:28:19 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
129     |2026-05-26 12:59:03 |Normal      |0x12000006  |Deasserted  |Chassis cover is open.
128     |2026-05-26 12:58:09 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
127     |2026-05-26 12:21:51 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
126     |2026-05-26 11:53:08 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
125     |2026-05-26 11:38:02 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
124     |2026-05-26 11:33:46 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
123     |2026-05-26 11:24:25 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
122     |2026-05-26 11:18:59 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
121     |2026-05-26 11:08:20 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
120     |2026-05-26 11:06:12 |Normal      |0x02000023  |Asserted    |The disk Disk0 is replaced from SN(2025082800559) to SN(S45RNC0T611284) (SN:S45RNC0T611284).
119     |2026-05-26 11:02:51 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
118     |2026-05-26 11:02:50 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
117     |2026-05-26 11:02:49 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
116     |2026-05-26 11:02:45 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
115     |2026-05-26 11:01:55 |Normal      |0x02000003  |Asserted    |The disk Disk0 installed.
114     |2026-05-26 10:54:13 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
113     |2026-05-26 10:54:11 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
112     |2026-05-26 10:54:05 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
111     |2026-05-26 10:53:58 |Normal      |0x02000023  |Asserted    |The disk Disk1 is replaced from SN(035MQBP0R8708785) to SN(2025082800559) (SN:2025082800559).
110     |2026-05-26 10:47:58 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
109     |2026-05-26 10:47:58 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
108     |2026-05-26 10:47:44 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
107     |2026-05-26 10:46:29 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-26 10:43:29 UTC, The power has been already restored.
106     |2026-05-26 10:45:03 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
105     |2026-05-26 10:44:53 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
104     |2026-05-26 10:44:49 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
103     |2026-05-26 10:42:52 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
102     |2026-05-26 10:42:50 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
101     |2026-05-26 10:42:43 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
100     |2026-05-26 10:36:59 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
99      |2026-05-26 10:34:37 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
98      |2026-05-26 10:34:36 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
97      |2026-05-26 10:34:34 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
96      |2026-05-26 10:34:34 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
95      |2026-05-26 10:34:31 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
94      |2026-05-26 10:34:29 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
93      |2026-05-26 10:34:23 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
92      |2026-05-26 10:33:50 |Normal      |0x02000023  |Asserted    |The disk Disk0 is replaced from SN(035MQBZER7012170) to SN(2025082800559) (SN:2025082800559).
91      |2026-05-26 10:29:23 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
90      |2026-05-26 09:48:05 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
89      |2026-05-26 09:48:05 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
88      |2026-05-26 09:48:03 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
87      |2026-05-26 09:48:01 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
86      |2026-05-26 09:47:57 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
85      |2026-05-26 09:47:56 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
84      |2026-05-26 09:47:49 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
83      |2026-05-26 09:45:36 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
82      |2026-05-26 09:42:33 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
81      |2026-05-26 09:42:33 |Normal      |0x2C000013  |Asserted    |The host was restarted by power button.
80      |2026-05-26 09:42:30 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
79      |2026-05-26 09:42:30 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
78      |2026-05-26 09:42:16 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
77      |2026-05-26 09:42:14 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
76      |2026-05-26 09:42:07 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
75      |2026-05-26 09:31:51 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
74      |2026-05-26 09:31:49 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
73      |2026-05-26 09:31:35 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
72      |2026-05-26 09:30:18 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-26 09:27:18 UTC, The power has been already restored.
71      |2026-05-26 09:28:54 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
70      |2026-05-26 09:28:42 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
69      |2026-05-26 09:28:40 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
68      |2026-05-26 09:26:03 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
67      |2026-05-26 09:25:55 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
66      |2026-05-26 09:25:52 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
65      |2026-05-26 09:25:41 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
64      |2026-05-26 09:25:39 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
63      |2026-05-26 09:20:24 |Normal      |0x31000002  |Deasserted  |The power button on the panel is pressed.
62      |2026-05-26 09:20:23 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
61      |2026-05-26 09:20:16 |Normal      |0x31000001  |Asserted    |The power button on the panel is pressed.
60      |2026-05-26 07:42:39 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-26 07:39:38 UTC, The power has been already restored.
59      |2026-05-26 07:41:34 |Normal      |0x12000006  |Deasserted  |Chassis cover is open.
58      |2026-05-26 07:41:32 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
57      |2026-05-26 07:41:14 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
56      |2026-05-26 07:41:00 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
55      |2026-05-26 07:40:59 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
54      |2026-05-25 08:58:46 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
53      |2026-05-25 08:53:35 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-18 06:13:22 UTC, The power has been already restored.
52      |2026-05-25 08:52:30 |Normal      |0x12000006  |Deasserted  |Chassis cover is open.
51      |2026-05-25 08:52:29 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
50      |2026-05-25 08:52:13 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
49      |2026-05-25 08:51:58 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
48      |2026-05-25 08:51:57 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
47      |2026-05-18 06:03:53 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
46      |2026-05-18 06:00:16 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
45      |2026-05-18 05:19:57 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-05-17 07:26:10 UTC, The power has been already restored.
44      |2026-05-18 05:18:30 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
43      |2026-05-18 05:18:21 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
42      |2026-05-18 05:18:17 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
41      |2026-05-17 07:04:22 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 2 disconnected.
40      |2026-05-17 07:04:22 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 1 disconnected.
39      |2026-05-17 07:04:15 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
38      |2026-05-17 06:34:51 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 2 disconnected.
37      |2026-05-17 06:34:51 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 1 disconnected.
36      |2026-05-17 06:33:51 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 2 disconnected.
35      |2026-05-17 06:33:51 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 1 disconnected.
34      |2026-05-17 06:33:12 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 2 disconnected.
33      |2026-05-17 06:33:12 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 1 disconnected.
32      |2026-05-17 06:31:56 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 2 disconnected.
31      |2026-05-17 06:31:56 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 1 disconnected.
30      |2026-05-17 06:31:48 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
29      |2026-05-17 05:51:25 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 2 disconnected.
28      |2026-05-17 05:51:25 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 1 disconnected.
27      |2026-05-17 05:48:57 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 2 disconnected.
26      |2026-05-17 05:48:57 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 1 disconnected.
25      |2026-05-17 05:47:30 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 2 disconnected.
24      |2026-05-17 05:47:30 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 1 disconnected.
23      |2026-05-17 05:46:14 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 2 disconnected.
22      |2026-05-17 05:46:13 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 1 disconnected.
21      |2026-05-17 05:46:00 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
20      |2026-05-17 05:45:40 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 2 disconnected.
19      |2026-05-17 05:45:40 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 1 disconnected.
18      |2026-05-17 05:44:26 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 2 disconnected.
17      |2026-05-17 05:44:26 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 1 disconnected.
16      |2026-05-17 05:44:16 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
15      |2026-05-17 03:09:38 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 2 disconnected.
14      |2026-05-17 03:09:38 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 1 disconnected.
13      |2026-05-17 03:07:10 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 2 disconnected.
12      |2026-05-17 03:07:10 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 1 disconnected.
11      |2026-05-17 03:04:37 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 2 disconnected.
10      |2026-05-17 03:04:36 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 1 disconnected.
9       |2026-05-17 03:03:20 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 2 disconnected.
8       |2026-05-17 03:03:20 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 1 disconnected.
7       |2026-05-17 03:03:08 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
6       |2026-05-17 02:34:18 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 2 disconnected.
5       |2026-05-17 02:34:18 |Normal      |0x29000002  |Deasserted  |NIC 1 (SF223D-H) Port 1 disconnected.
4       |2026-05-17 02:33:02 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 2 disconnected.
3       |2026-05-17 02:33:02 |Normal      |0x29000001  |Asserted    |NIC 1 (SF223D-H) Port 1 disconnected.
2       |2026-05-17 02:32:54 |Normal      |0x2C00000F  |Asserted    |The host was restarted due to unrecognized reason.
1       |2026-05-16 02:09:32 |Normal      |0x1A00000F  |Asserted    |iBMC event records are cleared.
