ID      |Generation Time     |Severity    |Event Code  |Status      |Event Description
31      |2026-02-06 08:01:42 |Minor       |0x08000006  |Deasserted  |Failed to obtain data of the OCP Card 1 (XC385) NICCard Chip temperature (SN:02Y238X6Q6000254, BN:0302Y238).
30      |2026-02-06 08:01:41 |Normal      |0x29000002  |Deasserted  |OCP Card 1 (XC385) Port 2 disconnected.
29      |2026-02-06 08:01:41 |Normal      |0x29000002  |Deasserted  |OCP Card 1 (XC385) Port 1 disconnected.
28      |2026-02-06 08:01:39 |Normal      |0x29000001  |Asserted    |OCP Card 1 (XC385) Port 1 disconnected.
27      |2026-02-06 07:52:37 |Minor       |0x08000005  |Asserted    |Failed to obtain data of the OCP Card 1 (XC385) NICCard Chip temperature (SN:02Y238X6Q6000254, BN:0302Y238).
26      |2026-02-06 06:22:01 |Normal      |0x29000001  |Asserted    |OCP Card 1 (XC385) Port 2 disconnected.
25      |2026-02-06 05:38:39 |Normal      |0x29000002  |Deasserted  |PCIe Card 3 (E610XT2M5) Port 1 disconnected.
24      |2026-02-06 05:38:34 |Normal      |0x29000002  |Deasserted  |PCIe Card 3 (E610XT2M5) Port 2 disconnected.
23      |2026-02-06 05:38:34 |Normal      |0x29000001  |Asserted    |PCIe Card 3 (E610XT2M5) Port 1 disconnected.
22      |2026-02-06 05:38:29 |Normal      |0x29000001  |Asserted    |PCIe Card 3 (E610XT2M5) Port 2 disconnected.
21      |2026-02-06 05:37:45 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-02-06 05:27:16 UTC, The power has been already restored.
20      |2026-02-06 05:36:17 |Major       |0x01000057  |Asserted    |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
19      |2026-02-06 05:35:43 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
18      |2026-02-06 05:35:29 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
17      |2026-02-06 05:35:05 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
16      |2026-02-06 05:35:01 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
15      |2026-02-06 03:19:48 |Minor       |0x08000006  |Deasserted  |Failed to obtain data of the OCP Card 1 (XC385) NICCard Chip temperature (SN:02Y238X6Q6000254, BN:0302Y238).
14      |2026-02-06 03:19:34 |Minor       |0x08000005  |Asserted    |Failed to obtain data of the OCP Card 1 (XC385) NICCard Chip temperature (SN:02Y238X6Q6000254, BN:0302Y238).
13      |2026-02-06 03:12:08 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
12      |2026-02-06 03:11:51 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
11      |2026-02-06 03:10:49 |Normal      |0x1A00006F  |Asserted    |The iBMC is reset, with the cause code of 0x1.
10      |2026-02-06 03:03:02 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
9       |2026-02-06 03:02:47 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
8       |2026-02-06 03:01:51 |Normal      |0x1A00006F  |Asserted    |The iBMC is reset, with the cause code of 0x2.
7       |2026-02-06 02:46:29 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
6       |2026-02-06 02:46:13 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
5       |2026-02-06 02:45:40 |Normal      |0x1A00006F  |Asserted    |The iBMC is reset, with the cause code of 0x1.
4       |2026-02-06 02:19:57 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
3       |2026-02-06 02:19:31 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
2       |2026-02-06 02:18:56 |Normal      |0x1A00006F  |Asserted    |The iBMC is reset, with the cause code of 0x2.
1       |2026-02-06 02:09:14 |Normal      |0x1A00000F  |Asserted    |iBMC event records are cleared.
