ID      |Generation Time     |Severity    |Event Code  |Status      |Event Description
56      |2026-02-28 08:23:38 |Minor       |0x08000006  |Deasserted  |Failed to obtain data of the OCP Card 2 (XC331) NICCard Chip temperature (SN:02Y237X6NB000029, BN:0302Y237).
55      |2026-02-28 08:22:11 |Minor       |0x08000005  |Asserted    |Failed to obtain data of the OCP Card 2 (XC331) NICCard Chip temperature (SN:02Y237X6NB000029, BN:0302Y237).
54      |2026-02-28 07:53:36 |Major       |0x01000057  |Asserted    |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
53      |2026-02-28 07:52:34 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
52      |2026-02-28 07:52:34 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
51      |2026-02-28 07:51:56 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-02-28 07:45:18 UTC, The power has been already restored.
50      |2026-02-28 07:49:26 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
49      |2026-02-28 07:49:06 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
48      |2026-02-28 07:27:21 |Major       |0x01000057  |Asserted    |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
47      |2026-02-28 07:26:19 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
46      |2026-02-28 07:26:19 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
45      |2026-02-28 07:20:03 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-02-28 07:10:14 UTC, The power has been already restored.
44      |2026-02-28 07:18:33 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
43      |2026-02-28 07:17:50 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
42      |2026-02-28 07:00:22 |Normal      |0x29000002  |Deasserted  |OCP Card 1 (XC331) Port 0 disconnected.
41      |2026-02-28 07:00:12 |Normal      |0x29000001  |Asserted    |OCP Card 1 (XC331) Port 0 disconnected.
40      |2026-02-28 07:00:02 |Normal      |0x29000002  |Deasserted  |OCP Card 1 (XC331) Port 1 disconnected.
39      |2026-02-28 06:59:57 |Normal      |0x29000001  |Asserted    |OCP Card 1 (XC331) Port 1 disconnected.
38      |2026-02-28 06:55:12 |Normal      |0x29000002  |Deasserted  |OCP Card 1 (XC331) Port 0 disconnected.
37      |2026-02-28 06:55:07 |Normal      |0x29000001  |Asserted    |OCP Card 1 (XC331) Port 0 disconnected.
36      |2026-02-28 06:54:57 |Normal      |0x29000002  |Deasserted  |OCP Card 1 (XC331) Port 0 disconnected.
35      |2026-02-28 06:54:42 |Normal      |0x29000001  |Asserted    |OCP Card 1 (XC331) Port 0 disconnected.
34      |2026-02-28 06:54:32 |Normal      |0x29000002  |Deasserted  |OCP Card 1 (XC331) Port 1 disconnected.
33      |2026-02-28 06:54:17 |Normal      |0x29000001  |Asserted    |OCP Card 1 (XC331) Port 1 disconnected.
32      |2026-02-28 06:26:51 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-02-28 06:16:38 UTC, The power has been already restored.
31      |2026-02-28 06:25:31 |Major       |0x01000057  |Asserted    |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
30      |2026-02-28 06:24:55 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
29      |2026-02-28 06:24:55 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
28      |2026-02-28 06:24:20 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
27      |2026-02-28 06:24:14 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
26      |2026-02-28 03:14:53 |Major       |0x01000057  |Asserted    |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
25      |2026-02-28 03:13:51 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
24      |2026-02-28 03:13:51 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
23      |2026-02-28 03:13:38 |Major       |0x01000058  |Deasserted  |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
22      |2026-02-28 03:13:37 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
21      |2026-02-28 03:07:13 |Major       |0x01000057  |Asserted    |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
20      |2026-02-28 03:06:12 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
19      |2026-02-28 03:06:11 |Major       |0x2C000008  |Deasserted  |The power EXU_V_12V0_FLEXIO1 failure results abnormal power-off.
18      |2026-02-28 03:06:11 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
17      |2026-02-28 03:05:59 |Major       |0x2C000007  |Asserted    |The power EXU_V_12V0_FLEXIO1 failure results abnormal power-off.
16      |2026-02-28 03:05:58 |Major       |0x01000058  |Deasserted  |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
15      |2026-02-28 03:05:57 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
14      |2026-02-28 03:01:21 |Major       |0x01000057  |Asserted    |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
13      |2026-02-28 03:00:22 |Normal      |0x2C000011  |Asserted    |The host was restarted by command.
12      |2026-02-28 03:00:19 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
11      |2026-02-28 02:37:19 |Major       |0x01000058  |Deasserted  |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
10      |2026-02-28 02:37:19 |Normal      |0x2C00000B  |Asserted    |ACPI is in the soft-off state.
9       |2026-02-28 02:01:24 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
8       |2026-02-28 02:01:09 |Normal      |0x1A000021  |Asserted    |iBMC is reset and started.
7       |2026-02-28 01:34:37 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-02-28 01:26:53 UTC, The power has been already restored.
6       |2026-02-28 01:33:18 |Major       |0x01000057  |Asserted    |DIMM100(CpuBoard1 DIMM100) memory initialization error. Error code: 0xEA14.
5       |2026-02-28 01:32:41 |Normal      |0x12000005  |Asserted    |Chassis cover is open.
4       |2026-02-28 01:32:27 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
3       |2026-02-28 01:32:03 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
2       |2026-02-28 01:31:59 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
1       |2026-02-28 01:27:05 |Normal      |0x1A00000F  |Asserted    |iBMC event records are cleared.
