ID      |Generation Time     |Severity    |Event Code  |Status      |Event Description
6       |2026-07-01 07:09:21 |Major       |0x28000033  |Asserted    |The cable of unit 00000001030302046571(SEUSlot5) is absent or the connector is not properly connected.
5       |2026-07-01 07:08:23 |Major       |0x0300001F  |Asserted    |Server power failure occurred at 2026-07-01 07:05:23 UTC, The power has been already restored.
4       |2026-07-01 07:06:04 |Normal      |0x2C000009  |Asserted    |ACPI is in the working state.
3       |2026-07-01 07:06:04 |Normal      |0x1A00000D  |Asserted    |iBMC is restarted after AC power supply is restored.
2       |2026-07-01 07:05:58 |Normal      |0x2C000017  |Asserted    |The host is restarted after being powered on (Power strategy is 'Turn On').
1       |2026-07-01 07:00:38 |Normal      |0x1A00000F  |Asserted    |iBMC event records are cleared.
