Gpio_31
└─Chip_Gpio_31_01

Gpio_56
└─Chip_Gpio_56_01

Gpio_74
└─Chip_Gpio_74_01

Hisport_0

Hisport_1

Hisport_10

Hisport_11

Hisport_12

Hisport_13

Hisport_14

Hisport_15

Hisport_16
└─Eeprom_3_5_010101

Hisport_17
└─Eeprom_3_6_010101

Hisport_18
├─Pca9545_PCA9545_01010101
│ ├─Channel_1
│ │ ├─Chip_RaidChip_0101010102
│ │ ├─Pca9555_Raid_0101010102
│ │ ├─Eeprom_Raid_0101010102
│ │ └─Lm75_Raid_0101010102
│ └─Channel_3
│   ├─Pca9555_IO_01010101
│   ├─Chip_MCU1_01010101
│   │ └─Channel_0
│   │   └─Eeprom_IEU_01010101
│   └─Lm75_LM75_01010101
└─Eeprom_3_1_010101

Hisport_19
└─Eeprom_3_2_010101

Hisport_2

Hisport_20
└─Eeprom_3_3_010101

Hisport_21
└─Eeprom_3_4_010101

Hisport_22

Hisport_23

Hisport_24

Hisport_25

Hisport_26

Hisport_27

Hisport_28

Hisport_29

Hisport_3

Hisport_30

Hisport_31

Hisport_32

Hisport_33

Hisport_34

Hisport_35

Hisport_36

Hisport_37

Hisport_38

Hisport_39

Hisport_4
└─Eeprom_3_10_010101

Hisport_40

Hisport_41

Hisport_42

Hisport_43

Hisport_44

Hisport_45

Hisport_46

Hisport_47

Hisport_48

Hisport_49

Hisport_5
└─Eeprom_3_7_010101

Hisport_50

Hisport_51

Hisport_52

Hisport_53

Hisport_54

Hisport_55

Hisport_56

Hisport_57

Hisport_58

Hisport_59

Hisport_6
└─Eeprom_3_12_010101

Hisport_60

Hisport_61

Hisport_62

Hisport_63

Hisport_7
└─Eeprom_3_11_010101

Hisport_8
└─Eeprom_3_8_010101

Hisport_9
└─Eeprom_3_9_010101

I2c_1
├─Eeprom_3_1_0101
├─Smc_CpuBrdSMC_0101
└─VChip_I2c_1

I2c_11
├─Lm75_OutletTemp_0101
└─VChip_I2c_11

I2c_2
├─Smc_ExpBoardSMC_0101
├─VChip_I2c_2
└─Eeprom_3_1_01

I2c_3
├─VChip_I2c_3
├─Eeprom_PsuChip1_0101
└─Eeprom_PsuChip2_0101

I2c_4
├─Smc_FanBoardSMC_0101
├─Eeprom_3_3_0101
└─VChip_I2c_4

I2c_5
├─VChip_I2c_5
├─Eeprom_3_2_0101
└─Smc_EnclSMC_010102
  ├─Channel_0
  │ ├─Eeprom_3_9_010102
  │ └─Smc_EnclSMC_01010209
  └─Channel_1
    └─Eeprom_3_10_010102

I2c_6
├─Pca9545_i2c6_chip_0101
│ ├─Channel_0
│ │ └─Eeprom_3_13_0101
│ └─Channel_2
│   ├─Eeprom_3_12_0101
│   ├─Smc_EnclSMC_01010C
│   │ └─Channel_1
│   │   ├─Chip_Virtual_SSD_01010C02
│   │   ├─Chip_Temp_01010C0201
│   │   └─Chip_SSD_01010C0201
│   └─Chip_Cpld_01010C
└─VChip_I2c_6

I2c_7
├─VChip_I2c_7
└─Pca9545_i2c7_chip_0101
  ├─Channel_0
  │ └─Eeprom_3_5_0101
  └─Channel_1
    └─Eeprom_3_6_0101

I2c_8
├─Eeprom_3_10_0101
├─Lm75_InletTemp_0101
├─Chip_UsbCc_Sgm_0101
├─Chip_UsbCc_On_0101
└─VChip_I2c_8

I2c_9

JtagOverLocalBus_1
└─JtagSwitch_1_0101
  ├─Channel_1
  │ └─Cpld_1_010101
  ├─Channel_2
  │ ├─Cpld_1_010102
  │ └─JtagSwitch_1_010102
  │   └─Channel_18
  │     └─Cpld_1_01010209
  ├─Channel_4
  │ └─Cpld_1_01010C
  ├─Channel_5
  │ └─Cpld_1_010103
  └─Channel_6
    └─Cpld_cpu_010101

Jtag_1
└─Cpld_1_0101


Chip alias:
Eeprom_EXU_0101 -> Eeprom_3_1_01
Smc_ExpBoardSMC_01010B -> Smc_ExpBoardSMC_0101
Smc_FanBoardSMC_01010305 -> Smc_FanBoardSMC_0101
Eeprom_1_01010A -> Eeprom_3_10_0101
Smc_ExpBoardSMC_01010A -> Smc_ExpBoardSMC_0101
Smc_CpuBrdSMC_01010118 -> Smc_CpuBrdSMC_0101
Smc_ExpBoardSMC_010109 -> Smc_ExpBoardSMC_0101
Chip_Temp_01010C0202 -> Chip_Temp_01010C0201
Smc_ExpBoardSMC_0101011C -> Smc_ExpBoardSMC_0101
Smc_CpuBrdSMC_0101011C -> Smc_CpuBrdSMC_0101
Smc_ExpBoardSMC_01010305 -> Smc_ExpBoardSMC_0101
Eeprom_SEU_01010C -> Eeprom_3_12_0101
Smc_ExpBoardSMC_010103 -> Smc_ExpBoardSMC_0101
Chip_Fan_PWM_010103 -> Smc_FanBoardSMC_0101
Smc_FanBoardSMC_01010303 -> Smc_FanBoardSMC_0101
Smc_ExpBoardSMC_010101 -> Smc_ExpBoardSMC_0101
Smc_ExpBoardSMC_01010303 -> Smc_ExpBoardSMC_0101
Smc_ExpBoardSMC_01010301 -> Smc_ExpBoardSMC_0101
Smc_FanBoardSMC_01010307 -> Smc_FanBoardSMC_0101
Smc_FanBoardSMC_01010301 -> Smc_FanBoardSMC_0101
Eeprom_BCU_010101 -> Eeprom_3_1_0101
Smc_ExpBoardSMC_01010C -> Smc_ExpBoardSMC_0101
Smc_ExpBoardSMC_01010209 -> Smc_ExpBoardSMC_0101
Smc_ExpBoardSMC_01010307 -> Smc_ExpBoardSMC_0101
Chip_Virtual_SSD_01010C0201 -> Chip_Virtual_SSD_01010C02
Eeprom_SEU_01010209 -> Eeprom_3_9_010102
Smc_CpuBrdSMC_010101 -> Smc_CpuBrdSMC_0101
Smc_ExpBoardSMC_010102 -> Smc_ExpBoardSMC_0101
Eeprom_SEU_010102 -> Eeprom_3_2_0101
Eeprom_CLU_010103 -> Eeprom_3_3_0101
Smc_FanBoardSMC_010103 -> Smc_FanBoardSMC_0101
